Modules | Macros
Defines
BLE Services » Human Input Device Service (HIDS)

## Modules
| Report Type values
| HIDS Report Type values define.
| Information Flags
| HIDS Information Flags define.

## Macros
#define | HIDS_CONNECTION_MAX
#define | HIDS_REPORT_MAX_SIZE 20
#define | HIDS_REPORT_MAP_MAX_SIZE 512

## Detailed Description

## Macro Definition Documentation

## ◆ HIDS_CONNECTION_MAX

#define HIDS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of Heart Rate Service connections.

## ◆ HIDS_REPORT_MAP_MAX_SIZE

#define HIDS_REPORT_MAP_MAX_SIZE 512

Limitation of length, as per Section 2.6.1 in HIDS Spec, version 1.0

## ◆ HIDS_REPORT_MAX_SIZE

#define HIDS_REPORT_MAX_SIZE 20

Maximum length of report.