Enumerations
Enumerations
Peripheral Driver » APP DRIVER » DUAL TIMER | Peripheral Driver » APP DRIVER » TIMER

## Enumerations
enum | app_dual_tim_id_t { APP_DUAL_TIM_ID_0, APP_DUAL_TIM_ID_1, APP_DUAL_TIM_ID_MAX }
| APP_DUAL_TIM module Enumerations definition. More...
enum | app_dual_tim_evt_t { APP_DUAL_TIM_EVT_ERROR, APP_DUAL_TIM_EVT_DONE }
| DUAL_TIM event Enumerations definition. More...
enum | app_tim_id_t { APP_TIM_ID_0, APP_TIM_ID_1, APP_TIM_ID_MAX }
| TIM module Enumerations definition. More...
enum | app_tim_evt_t { APP_TIM_EVT_ERROR, APP_TIM_EVT_DONE }
| TIM event Enumerations definition. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ app_dual_tim_evt_t

enum app_dual_tim_evt_t

DUAL_TIM event Enumerations definition.

Enumerator
APP_DUAL_TIM_EVT_ERROR | Error reported by DUAL TIMER peripheral.
APP_DUAL_TIM_EVT_DONE | Interrupt done by DUAL TIMER peripheral.

## ◆ app_dual_tim_id_t

enum app_dual_tim_id_t

APP_DUAL_TIM module Enumerations definition.

Enumerator
APP_DUAL_TIM_ID_0 | DUAL TIMER module 0
APP_DUAL_TIM_ID_1 | DUAL TIMER module 1
APP_DUAL_TIM_ID_MAX | Only for check parameter, not used as input parameters.

## ◆ app_tim_evt_t

enum app_tim_evt_t

TIM event Enumerations definition.

Enumerator
APP_TIM_EVT_ERROR | Error reported by TIMER peripheral.
APP_TIM_EVT_DONE | Interrupt done by TIMER peripheral.

## ◆ app_tim_id_t

enum app_tim_id_t

TIM module Enumerations definition.

Enumerator
APP_TIM_ID_0 | TIMER module 0
APP_TIM_ID_1 | TIMER module 1
APP_TIM_ID_MAX | Only for check parameter, not used as input parameters.