Data Fields
hids_evt_t Struct Reference
BLE Services » Human Input Device Service (HIDS) » Typedefs

HID Service event. More...

`#include <hids.h>`

## Data Fields
hids_evt_type_t | evt_type
uint8_t | conn_idx
hids_report_type_t | report_type
uint16_t | offset
uint16_t | len
uint8_t const * | data

## Detailed Description

HID Service event.

## Field Documentation

## ◆ conn_idx

uint8_t hids_evt_t::conn_idx

Connect index.

## ◆ data

uint8_t const* hids_evt_t::data

Incoming data, variable length

## ◆ evt_type

hids_evt_type_t hids_evt_t::evt_type

Type of event.

## ◆ len

uint16_t hids_evt_t::len

Length of the incoming data.

## ◆ offset

uint16_t hids_evt_t::offset

Offset for the write operation.

## ◆ report_type

hids_report_type_t hids_evt_t::report_type

Type of report, see hids_report_type_t.

The documentation for this struct was generated from the following file:

- hids.h