Macros
EFUSE Flags
Peripheral Driver » HAL Driver » EFUSE » Defines » EFUSE Exported Macros

## Macros
#define | EFUSE_FLAG_WRITE_KEYRAM_BUSY LL_EFUSE_WRITE_KEYRAM_BUSY
#define | EFUSE_FLAG_READ_TRIM_DONE LL_EFUSE_READ_TRIM_DONE
#define | EFUSE_FLAG_CRC_CHECK_DONE LL_EFUSE_CRC_CHECK_DONE
#define | EFUSE_FLAG_CRC_CHECK_SUCCESS LL_EFUSE_CRC_CHECK_SUCCESS
#define | EFUSE_FLAG_INIT_CHECK_DONE LL_EFUSE_INIT_CHECK_DONE
#define | EFUSE_FLAG_INIT_CHECK_SUCCESS LL_EFUSE_INIT_CHECK_SUCCESS
#define | EFUSE_FLAG_WRITE_DONE LL_EFUSE_WRITE_DONE
#define | EFUSE_FLAG_TEST_DONE LL_EFUSE_TEST_DONE

## Detailed Description

## Macro Definition Documentation

## ◆ EFUSE_FLAG_CRC_CHECK_DONE

#define EFUSE_FLAG_CRC_CHECK_DONE LL_EFUSE_CRC_CHECK_DONE

eFuse CRC check done

## ◆ EFUSE_FLAG_CRC_CHECK_SUCCESS

#define EFUSE_FLAG_CRC_CHECK_SUCCESS LL_EFUSE_CRC_CHECK_SUCCESS

CRC check succeeded

## ◆ EFUSE_FLAG_INIT_CHECK_DONE

#define EFUSE_FLAG_INIT_CHECK_DONE LL_EFUSE_INIT_CHECK_DONE

eFuse initial value check done

## ◆ EFUSE_FLAG_INIT_CHECK_SUCCESS

#define EFUSE_FLAG_INIT_CHECK_SUCCESS LL_EFUSE_INIT_CHECK_SUCCESS

eFuse initial value check succeeded

## ◆ EFUSE_FLAG_READ_TRIM_DONE

#define EFUSE_FLAG_READ_TRIM_DONE LL_EFUSE_READ_TRIM_DONE

Read trim from eFuse has done

## ◆ EFUSE_FLAG_TEST_DONE

#define EFUSE_FLAG_TEST_DONE LL_EFUSE_TEST_DONE

Read from eFuse has done in test mode

## ◆ EFUSE_FLAG_WRITE_DONE

#define EFUSE_FLAG_WRITE_DONE LL_EFUSE_WRITE_DONE

eFuse one word write done

## ◆ EFUSE_FLAG_WRITE_KEYRAM_BUSY

#define EFUSE_FLAG_WRITE_KEYRAM_BUSY LL_EFUSE_WRITE_KEYRAM_BUSY

Write keyram operation is in process