Macros
IO States Defines
Peripheral Driver » LL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | LL_ISO7816_IO_STATE_OFF (0x0UL << ISO7816_STAT_IO_STAT_POS)
#define | LL_ISO7816_IO_STATE_IDLE (0x1UL << ISO7816_STAT_IO_STAT_POS)
#define | LL_ISO7816_IO_STATE_RX_WAIT (0x4UL << ISO7816_STAT_IO_STAT_POS)
#define | LL_ISO7816_IO_STATE_RX (0x5UL << ISO7816_STAT_IO_STAT_POS)
#define | LL_ISO7816_IO_STATE_TX (0x6UL << ISO7816_STAT_IO_STAT_POS)
#define | LL_ISO7816_IO_STATE_TX_GUARD (0x7UL << ISO7816_STAT_IO_STAT_POS)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_ISO7816_IO_STATE_IDLE

#define LL_ISO7816_IO_STATE_IDLE (0x1UL << ISO7816_STAT_IO_STAT_POS)

Idle

## ◆ LL_ISO7816_IO_STATE_OFF

#define LL_ISO7816_IO_STATE_OFF (0x0UL << ISO7816_STAT_IO_STAT_POS)

Off

## ◆ LL_ISO7816_IO_STATE_RX

#define LL_ISO7816_IO_STATE_RX (0x5UL << ISO7816_STAT_IO_STAT_POS)

Receive

## ◆ LL_ISO7816_IO_STATE_RX_WAIT

#define LL_ISO7816_IO_STATE_RX_WAIT (0x4UL << ISO7816_STAT_IO_STAT_POS)

Receive Wait

## ◆ LL_ISO7816_IO_STATE_TX

#define LL_ISO7816_IO_STATE_TX (0x6UL << ISO7816_STAT_IO_STAT_POS)

Transmit

## ◆ LL_ISO7816_IO_STATE_TX_GUARD

#define LL_ISO7816_IO_STATE_TX_GUARD (0x7UL << ISO7816_STAT_IO_STAT_POS)

Transmit Guard