Macros
DMA Priority Level
Peripheral Driver » HAL Driver » DMA » Defines » DMA Exported Constants

## Macros
#define | DMA_PRIORITY_LOW LL_DMA_PRIORITY_0
#define | DMA_PRIORITY_MEDIUM LL_DMA_PRIORITY_2
#define | DMA_PRIORITY_HIGH LL_DMA_PRIORITY_5
#define | DMA_PRIORITY_VERY_HIGH LL_DMA_PRIORITY_7

## Detailed Description

## Macro Definition Documentation

## ◆ DMA_PRIORITY_HIGH

#define DMA_PRIORITY_HIGH LL_DMA_PRIORITY_5

Priority level : High

## ◆ DMA_PRIORITY_LOW

#define DMA_PRIORITY_LOW LL_DMA_PRIORITY_0

Priority level : Low

## ◆ DMA_PRIORITY_MEDIUM

#define DMA_PRIORITY_MEDIUM LL_DMA_PRIORITY_2

Priority level : Medium

## ◆ DMA_PRIORITY_VERY_HIGH

#define DMA_PRIORITY_VERY_HIGH LL_DMA_PRIORITY_7

Priority level : Very High