Macros
DFU cmd disable option (bitmask)
SYSTEM » Device Firmware Update » Defines

## Macros
#define | DFU_WRITE_RAM_DISABLE 0x0001
#define | DFU_READ_RAM_DISABLE 0x0002
#define | DFU_DUMP_FLASH_DISABLE 0x0004
#define | DFU_ERASE_FLASH_DISABLE 0x0008
#define | DFU_UPDAE_FLASH_DISABLE 0x0010
#define | DFU_OPERATE_SYSTEM_INFO_DISABLE 0x0020
#define | DFU_OPERATE_NVDS_DISABLE 0x0040
#define | DFU_OPERATE_EFUSE_DISABLE 0x0080
#define | DFU_CONFIG_SPI_FLASH_DISABLE 0x0100
#define | DFU_OPERATE_REG_DISABLE 0x0200

## Detailed Description

## Macro Definition Documentation

## ◆ DFU_CONFIG_SPI_FLASH_DISABLE

#define DFU_CONFIG_SPI_FLASH_DISABLE 0x0100

Disable DFU config spi flash.

## ◆ DFU_DUMP_FLASH_DISABLE

#define DFU_DUMP_FLASH_DISABLE 0x0004

Disable DFU dump flash.

## ◆ DFU_ERASE_FLASH_DISABLE

#define DFU_ERASE_FLASH_DISABLE 0x0008

Disable DFU erase flash.

## ◆ DFU_OPERATE_EFUSE_DISABLE

#define DFU_OPERATE_EFUSE_DISABLE 0x0080

Disable DFU operate EFUSE.

## ◆ DFU_OPERATE_NVDS_DISABLE

#define DFU_OPERATE_NVDS_DISABLE 0x0040

Disable DFU operate NVDS.

## ◆ DFU_OPERATE_REG_DISABLE

#define DFU_OPERATE_REG_DISABLE 0x0200

Disable DFU operate register.

## ◆ DFU_OPERATE_SYSTEM_INFO_DISABLE

#define DFU_OPERATE_SYSTEM_INFO_DISABLE 0x0020

Disable DFU operate system info area.

## ◆ DFU_READ_RAM_DISABLE

#define DFU_READ_RAM_DISABLE 0x0002

Disable DFU read ram.

## ◆ DFU_UPDAE_FLASH_DISABLE

#define DFU_UPDAE_FLASH_DISABLE 0x0010

Disable DFU update flash.

## ◆ DFU_WRITE_RAM_DISABLE

#define DFU_WRITE_RAM_DISABLE 0x0001

Disable DFU write ram.