Macros
EFUSE Operation Defines
Peripheral Driver » LL Driver » EFUSE » Defines » EFUSE Exported Constants

Operation defines which can be used with LL_EFUSE_WriteReg function. More...

## Macros
#define | LL_EFUSE_WRITE_KEYRAM EFUSE_OPER_WRITE_KEYRAM
#define | LL_EFUSE_READ_TRIM EFUSE_OPER_READ_TRIM
#define | LL_EFUSE_CRC_CHECK EFUSE_OPER_CRC_CHECK
#define | LL_EFUSE_INIT_CHECK EFUSE_OPER_INIT_CHECK
#define | LL_EFUSE_TEST_READ EFUSE_OPER_RD_TEST_MODE

## Detailed Description

Operation defines which can be used with LL_EFUSE_WriteReg function.

## Macro Definition Documentation

## ◆ LL_EFUSE_CRC_CHECK

#define LL_EFUSE_CRC_CHECK EFUSE_OPER_CRC_CHECK

Read the special eFuse addr, and calculate CRC value

## ◆ LL_EFUSE_INIT_CHECK

#define LL_EFUSE_INIT_CHECK EFUSE_OPER_INIT_CHECK

Read the whole eFuse value, and check this value with 0

## ◆ LL_EFUSE_READ_TRIM

#define LL_EFUSE_READ_TRIM EFUSE_OPER_READ_TRIM

Read analog trim from eFuse

## ◆ LL_EFUSE_TEST_READ

#define LL_EFUSE_TEST_READ EFUSE_OPER_RD_TEST_MODE

Read eFuse test mode from eFuse

## ◆ LL_EFUSE_WRITE_KEYRAM

#define LL_EFUSE_WRITE_KEYRAM EFUSE_OPER_WRITE_KEYRAM

Read fwkay and rootkey from eFuse, and write to keyram