Macros
Current Time Adjust Reason
BLE Services » Current Time Service Client (CTS_C) » Defines

Current Time Service Adjust Reason. More...

## Macros
#define | CTS_C_AR_NO_CHANGE (0x00 << 0)
#define | CTS_C_AR_MAUAL_TIME_UPDATE (0x01 << 0)
#define | CTS_C_AR_EXT_REF_TIME_UPDATE (0x01 << 1)
#define | CTS_C_AR_TIME_ZONE_CHANGE (0x01 << 2)
#define | CTS_C_AR_DST_CHANGE (0x01 << 3)

## Detailed Description

Current Time Service Adjust Reason.

## Macro Definition Documentation

## ◆ CTS_C_AR_DST_CHANGE

#define CTS_C_AR_DST_CHANGE (0x01 << 3)

Change of DST (daylight savings time).

## ◆ CTS_C_AR_EXT_REF_TIME_UPDATE

#define CTS_C_AR_EXT_REF_TIME_UPDATE (0x01 << 1)

External reference time update.

## ◆ CTS_C_AR_MAUAL_TIME_UPDATE

#define CTS_C_AR_MAUAL_TIME_UPDATE (0x01 << 0)

Manual time update.

## ◆ CTS_C_AR_NO_CHANGE

#define CTS_C_AR_NO_CHANGE (0x00 << 0)

No change for current time.

## ◆ CTS_C_AR_TIME_ZONE_CHANGE

#define CTS_C_AR_TIME_ZONE_CHANGE (0x01 << 2)

Change of time zone.