Enumerations
Measurement Flag Bits
BLE Services » Weight Scale Service (WSS)

Weight Scale Measurement Flags. More...

Collaboration diagram for Measurement Flag Bits:

## Enumerations
enum | wss_meas_flag_bits { WSS_MEAS_FLAG_UNIT_SI = 0x00, WSS_MEAS_FLAG_UNIT_IMPERIAL = 0x01, WSS_MEAS_FLAG_DATE_TIME_PRESENT = 0x02, WSS_MEAS_FLAG_USER_ID_PRESENT = 0x04, WSS_MEAS_FLAG_BMI_HEIGHT_PRESENT = 0x08 }

## Detailed Description

Weight Scale Measurement Flags.

## Enumeration Type Documentation

## ◆ wss_meas_flag_bits

enum wss_meas_flag_bits

Enumerator
WSS_MEAS_FLAG_UNIT_SI | Flag bit for SI Measurement Units Present.
WSS_MEAS_FLAG_UNIT_IMPERIAL | Flag bit for Imperial Measurement Units Present.
WSS_MEAS_FLAG_DATE_TIME_PRESENT | Flag bit for Time Stamp Present.
WSS_MEAS_FLAG_USER_ID_PRESENT | Flag bit for User ID Present.
WSS_MEAS_FLAG_BMI_HEIGHT_PRESENT | Flag bit for BMI and Height Present.