Macros
Get Flags Defines
Peripheral Driver » LL Driver » EFUSE » Defines » EFUSE Exported Constants

Flags defines which can be used with LL_EFUSE_ReadReg function. More...

## Macros
#define | LL_EFUSE_WRITE_KEYRAM_BUSY EFUSE_STATUS_WRITE_KEYRAM_BUSY
#define | LL_EFUSE_READ_TRIM_DONE EFUSE_STATUS_READ_TRIM_DONE
#define | LL_EFUSE_CRC_CHECK_DONE EFUSE_STATUS_CRC_CHECK_DONE
#define | LL_EFUSE_CRC_CHECK_SUCCESS EFUSE_STATUS_TRIM_CRC_SUCCESS
#define | LL_EFUSE_INIT_CHECK_DONE EFUSE_STATUS_INIT_DONE
#define | LL_EFUSE_INIT_CHECK_SUCCESS EFUSE_STATUS_INIT_SUCCESS
#define | LL_EFUSE_WRITE_DONE EFUSE_STATUS_WRITE_DONE
#define | LL_EFUSE_TEST_DONE EFUSE_STATUS_TEST_MODE_DONE

## Detailed Description

Flags defines which can be used with LL_EFUSE_ReadReg function.

## Macro Definition Documentation

## ◆ LL_EFUSE_CRC_CHECK_DONE

#define LL_EFUSE_CRC_CHECK_DONE EFUSE_STATUS_CRC_CHECK_DONE

eFuse CRC check done

## ◆ LL_EFUSE_CRC_CHECK_SUCCESS

#define LL_EFUSE_CRC_CHECK_SUCCESS EFUSE_STATUS_TRIM_CRC_SUCCESS

CRC check success

## ◆ LL_EFUSE_INIT_CHECK_DONE

#define LL_EFUSE_INIT_CHECK_DONE EFUSE_STATUS_INIT_DONE

eFuse initial value check done

## ◆ LL_EFUSE_INIT_CHECK_SUCCESS

#define LL_EFUSE_INIT_CHECK_SUCCESS EFUSE_STATUS_INIT_SUCCESS

eFuse initial value check success

## ◆ LL_EFUSE_READ_TRIM_DONE

#define LL_EFUSE_READ_TRIM_DONE EFUSE_STATUS_READ_TRIM_DONE

Read trim from eFuse has done

## ◆ LL_EFUSE_TEST_DONE

#define LL_EFUSE_TEST_DONE EFUSE_STATUS_TEST_MODE_DONE

Read from eFuse has done in test mode

## ◆ LL_EFUSE_WRITE_DONE

#define LL_EFUSE_WRITE_DONE EFUSE_STATUS_WRITE_DONE

eFuse one word write done

## ◆ LL_EFUSE_WRITE_KEYRAM_BUSY

#define LL_EFUSE_WRITE_KEYRAM_BUSY EFUSE_STATUS_WRITE_KEYRAM_BUSY

Write keyram operation is in processing