Macros
Operation Mode
Peripheral Driver » LL Driver » PKC » Defines » PKC Exported Constants

## Macros
#define | LL_PKC_operation_mode_MULTIPLY (0x00000000U)
#define | LL_PKC_operation_mode_INVERTION (1UL << PKC_SW_CTRL_OPMODE_Pos)
#define | LL_PKC_operation_mode_ADD (2UL << PKC_SW_CTRL_OPMODE_Pos)
#define | LL_PKC_operation_mode_SUB (3UL << PKC_SW_CTRL_OPMODE_Pos)
#define | LL_PKC_operation_mode_COMPARE (4UL << PKC_SW_CTRL_OPMODE_Pos)
#define | LL_PKC_operation_mode_LEFTSHIFT (5UL << PKC_SW_CTRL_OPMODE_Pos)
#define | LL_PKC_operation_mode_BIGINTEGERMULTIPLY (6UL << PKC_SW_CTRL_OPMODE_Pos)
#define | LL_PKC_operation_mode_BIGINTEGERADD (7UL << PKC_SW_CTRL_OPMODE_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_PKC_operation_mode_ADD

#define LL_PKC_operation_mode_ADD (2UL << PKC_SW_CTRL_OPMODE_Pos)

Addition operation mode

## ◆ LL_PKC_operation_mode_BIGINTEGERADD

#define LL_PKC_operation_mode_BIGINTEGERADD (7UL << PKC_SW_CTRL_OPMODE_Pos)

Big Number Addition operation mode

## ◆ LL_PKC_operation_mode_BIGINTEGERMULTIPLY

#define LL_PKC_operation_mode_BIGINTEGERMULTIPLY (6UL << PKC_SW_CTRL_OPMODE_Pos)

Big Number Multiplication operation mode

## ◆ LL_PKC_operation_mode_COMPARE

#define LL_PKC_operation_mode_COMPARE (4UL << PKC_SW_CTRL_OPMODE_Pos)

Comparison operation mode

## ◆ LL_PKC_operation_mode_INVERTION

#define LL_PKC_operation_mode_INVERTION (1UL << PKC_SW_CTRL_OPMODE_Pos)

Inversion operation mode

## ◆ LL_PKC_operation_mode_LEFTSHIFT

#define LL_PKC_operation_mode_LEFTSHIFT (5UL << PKC_SW_CTRL_OPMODE_Pos)

Left Shift operation mode

## ◆ LL_PKC_operation_mode_MULTIPLY

#define LL_PKC_operation_mode_MULTIPLY (0x00000000U)

Multiplication operation mode

## ◆ LL_PKC_operation_mode_SUB

#define LL_PKC_operation_mode_SUB (3UL << PKC_SW_CTRL_OPMODE_Pos)

Subtraction operation mode