Macros
Power States Defines
Peripheral Driver » HAL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | HAL_ISO7816_PWR_STATE_OFF LL_ISO7816_PWR_STATE_OFF
#define | HAL_ISO7816_PWR_STATE_PWRUP_VCC LL_ISO7816_PWR_STATE_PWRUP_VCC
#define | HAL_ISO7816_PWR_STATE_PWRUP_RST LL_ISO7816_PWR_STATE_PWRUP_RST
#define | HAL_ISO7816_PWR_STATE_PWRDN_RST LL_ISO7816_PWR_STATE_PWRDN_RST
#define | HAL_ISO7816_PWR_STATE_PWRDN_VCC LL_ISO7816_PWR_STATE_PWRDN_VCC
#define | HAL_ISO7816_PWR_STATE_STOP_PRE LL_ISO7816_PWR_STATE_STOP_PRE
#define | HAL_ISO7816_PWR_STATE_STOP LL_ISO7816_PWR_STATE_STOP
#define | HAL_ISO7816_PWR_STATE_STOP_POST LL_ISO7816_PWR_STATE_STOP_POST
#define | HAL_ISO7816_PWR_STATE_IDLE LL_ISO7816_PWR_STATE_IDLE
#define | HAL_ISO7816_PWR_STATE_RX_TS0 LL_ISO7816_PWR_STATE_RX_TS0
#define | HAL_ISO7816_PWR_STATE_RX_TS1 LL_ISO7816_PWR_STATE_RX_TS1
#define | HAL_ISO7816_PWR_STATE_RX LL_ISO7816_PWR_STATE_RX
#define | HAL_ISO7816_PWR_STATE_TX LL_ISO7816_PWR_STATE_TX
#define | HAL_ISO7816_PWR_STATE_TX_RX LL_ISO7816_PWR_STATE_TX_RX

## Detailed Description

## Macro Definition Documentation

## ◆ HAL_ISO7816_PWR_STATE_IDLE

#define HAL_ISO7816_PWR_STATE_IDLE LL_ISO7816_PWR_STATE_IDLE

Idle

## ◆ HAL_ISO7816_PWR_STATE_OFF

#define HAL_ISO7816_PWR_STATE_OFF LL_ISO7816_PWR_STATE_OFF

Off

## ◆ HAL_ISO7816_PWR_STATE_PWRDN_RST

#define HAL_ISO7816_PWR_STATE_PWRDN_RST LL_ISO7816_PWR_STATE_PWRDN_RST

Power Down reset

## ◆ HAL_ISO7816_PWR_STATE_PWRDN_VCC

#define HAL_ISO7816_PWR_STATE_PWRDN_VCC LL_ISO7816_PWR_STATE_PWRDN_VCC

Power Down VCC

## ◆ HAL_ISO7816_PWR_STATE_PWRUP_RST

#define HAL_ISO7816_PWR_STATE_PWRUP_RST LL_ISO7816_PWR_STATE_PWRUP_RST

Power up reset

## ◆ HAL_ISO7816_PWR_STATE_PWRUP_VCC

#define HAL_ISO7816_PWR_STATE_PWRUP_VCC LL_ISO7816_PWR_STATE_PWRUP_VCC

Power up VCC

## ◆ HAL_ISO7816_PWR_STATE_RX

#define HAL_ISO7816_PWR_STATE_RX LL_ISO7816_PWR_STATE_RX

Receive

## ◆ HAL_ISO7816_PWR_STATE_RX_TS0

#define HAL_ISO7816_PWR_STATE_RX_TS0 LL_ISO7816_PWR_STATE_RX_TS0

RX TS Character

## ◆ HAL_ISO7816_PWR_STATE_RX_TS1

#define HAL_ISO7816_PWR_STATE_RX_TS1 LL_ISO7816_PWR_STATE_RX_TS1

RX TS Character

## ◆ HAL_ISO7816_PWR_STATE_STOP

#define HAL_ISO7816_PWR_STATE_STOP LL_ISO7816_PWR_STATE_STOP

Clock Stopped

## ◆ HAL_ISO7816_PWR_STATE_STOP_POST

#define HAL_ISO7816_PWR_STATE_STOP_POST LL_ISO7816_PWR_STATE_STOP_POST

Exiting Clock Stop

## ◆ HAL_ISO7816_PWR_STATE_STOP_PRE

#define HAL_ISO7816_PWR_STATE_STOP_PRE LL_ISO7816_PWR_STATE_STOP_PRE

Preparing Clock Stop

## ◆ HAL_ISO7816_PWR_STATE_TX

#define HAL_ISO7816_PWR_STATE_TX LL_ISO7816_PWR_STATE_TX

Transmit

## ◆ HAL_ISO7816_PWR_STATE_TX_RX

#define HAL_ISO7816_PWR_STATE_TX_RX LL_ISO7816_PWR_STATE_TX_RX

Transmit and Receive