Macros
Feature Bits
BLE Services » Cycling Speed and Cadence Service (CSCS) » Defines

Cycling Speed and Cadence Service feature bits. More...

## Macros
#define | CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT (0x01 << 0)
#define | CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT (0x01 << 1)
#define | CSCS_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 2)
#define | CSCS_FEAR_FULL_BIT (0x07)

## Detailed Description

Cycling Speed and Cadence Service feature bits.

## Macro Definition Documentation

## ◆ CSCS_FEAR_FULL_BIT

#define CSCS_FEAR_FULL_BIT (0x07)

Bit for all CSC features Supported.

## ◆ CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT

#define CSCS_FEAT_CRANK_REVOLUTION_SUP_BIT (0x01 << 1)

Bit for Crank Revolution Data Supported.

## ◆ CSCS_FEAT_MULTIPLE_SENSORS_BIT

#define CSCS_FEAT_MULTIPLE_SENSORS_BIT (0x01 << 2)

Bit for Multiple Sensor Locations Supported.

## ◆ CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT

#define CSCS_FEAT_WHEEL_REVOLUTION_SUP_BIT (0x01 << 0)

Bit for Wheel Revolution Data Supported.