Modules | Macros
Defines
BLE Services » Weight Scale Service (WSS)

## Modules
| Characteristics Mask
| Bit masks for the initialization of wss_init_t::char_mask.

## Macros
#define | WSS_CONNECTION_MAX
#define | WSS_MEAS_VAL_LEN_MAX 15
#define | WSS_CACHE_MEAS_NUM_MAX 25
#define | WSS_FEAT_VAL_LEN_MAX 1
#define | WSS_MEAS_UNSUCCESS 0xFFFF

## Detailed Description

## Macro Definition Documentation

## ◆ WSS_CACHE_MEAS_NUM_MAX

#define WSS_CACHE_MEAS_NUM_MAX 25

Maximum number of cache muasurements value for each user.

## ◆ WSS_CONNECTION_MAX

#define WSS_CONNECTION_MAX

Value:
(10 < CFG_MAX_CONNECTIONS ?\
10 : CFG_MAX_CONNECTIONS)

Maximum number of Weight Scale Service connections.

## ◆ WSS_FEAT_VAL_LEN_MAX

#define WSS_FEAT_VAL_LEN_MAX 1

Maximum length of WS Feature value.

## ◆ WSS_MEAS_UNSUCCESS

#define WSS_MEAS_UNSUCCESS 0xFFFF

Measurement Unsuccessful.

## ◆ WSS_MEAS_VAL_LEN_MAX

#define WSS_MEAS_VAL_LEN_MAX 15

Maximum length of Weight Measurment value.