Data Structures | Macros | Typedefs | Enumerations | Functions
pass.h File Reference

Phone Alert Status Service API. More...

`#include "gr55xx_sys.h"`
`#include "custom_config.h"`
`#include <stdint.h>`
`#include <stdbool.h>`

Go to the source code of this file.

## Data Structures
struct | pass_evt_t
| Phone Alert Status Service event. More...
struct | pass_init_t
| Phone Alert Status Service init stucture. This contains all option and data needed for initialization of the service. More...

## Macros
#define | PASS_CONNECTION_MAX
#define | PASS_ALERT_STATUS_VAL_LEN 1
#define | PASS_RINGER_SET_VAL_LEN 1
#define | PASS_RINGER_CTRL_PT_VAL_LEN 1
#define | PASS_CHAR_MANDATORY 0x003f
#define | PASS_CHAR_RING_CTRL_PT_SUP 0x0180
#define | PASS_CHAR_FULL 0x01ff
#define | PASS_NO_STATE_ACTIVE (0x00)
#define | PASS_RINGER_ACTIVE (0x01 << 0)
#define | PASS_VIBRATE_ACTIVE (0x01 << 1)
#define | PASS_DISPLAY_ALERT_ACTIVE (0x01 << 2)
#define | PASS_ALL_STATE_ACTIVE (0x07)
#define | PASS_RINGER_SET_SILENT 0
#define | PASS_RINGER_SET_NORMAL 1

## Typedefs
typedef void(* | pass_evt_handler_t) (pass_evt_t *p_evt)
| Phone Alert Status Service event handler type.

## Enumerations
enum | pass_ringer_ctrl_pt_t { PASS_CTRL_PT_SILENT_MODE = 0x01, PASS_CTRL_PT_MUTE_ONCE, PASS_CTRL_PT_CANCEL_SLIENT_MODE }
| Phone Alert Status Service Ringer Control Point. More...
enum | pass_evt_type_t { PASS_EVT_INVALID, PASS_EVT_ALERT_STATUS_NTF_ENABLE, PASS_EVT_ALERT_STATUS_NTF_DISABLE, PASS_EVT_RINGER_SET_NTF_ENABLE, PASS_EVT_RINGER_SET_NTF_DISABLE, PASS_EVT_SILENT_MODE_SET, PASS_EVT_MUTE_ONCE_SET, PASS_EVT_SILENT_MODE_CANCEL }
| Phone Alert Status Service event type. More...

## Functions
sdk_err_t | pass_service_init (pass_init_t *p_pass_init)
| Initialize a Phone Alert Status Service instance and add in the DB. More...
uint8_t | pass_ringer_setting_get (void)
| Get Ringer Setting value. More...
void | pass_ringer_setting_set (uint8_t conn_idx, uint8_t new_setting)
| Set Ringer Setting value. More...
void | pass_alert_status_set (uint8_t conn_idx, uint8_t new_status)
| Set Alert Status value. More...

## Detailed Description

Phone Alert Status Service API.

Attention

  ##### Copyright (c) 2019 GOODIX

All rights reserved.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of GOODIX nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.