Functions
IT_Management
Peripheral Driver » LL Driver » PKC » Functions

## Functions
__STATIC_INLINE void | ll_pkc_enable_it_done (pkc_regs_t *PKCx)
| Enable the operation done interrupt. More...
__STATIC_INLINE void | ll_pkc_enable_it_err (pkc_regs_t *PKCx)
| Enable the operation error interrupt. More...
__STATIC_INLINE void | ll_pkc_enable_it_big_add_overflow (pkc_regs_t *PKCx)
| Enable the big integer overflow interrupt. More...
__STATIC_INLINE void | ll_pkc_disable_it_done (pkc_regs_t *PKCx)
| Disable the operation done interrupt. More...
__STATIC_INLINE void | ll_pkc_disable_it_err (pkc_regs_t *PKCx)
| Disable the operation error interrupt. More...
__STATIC_INLINE void | ll_pkc_disable_it_big_add_overflow (pkc_regs_t *PKCx)
| Disable the big integer overflow interrupt. More...
__STATIC_INLINE uint32_t | ll_pkc_is_enable_it_done (pkc_regs_t *PKCx)
| Indicate whether the operation done interrupt is enable. More...
__STATIC_INLINE uint32_t | ll_pkc_is_enable_it_err (pkc_regs_t *PKCx)
| Indicate whether the operation error interrupt is enable. More...
__STATIC_INLINE uint32_t | ll_pkc_is_enable_it_big_add_overflow (pkc_regs_t *PKCx)
| Indicate whether the big integer overflow interrupt is enable. More...

## Detailed Description

## Function Documentation

## ◆ ll_pkc_disable_it_big_add_overflow()

__STATIC_INLINE void ll_pkc_disable_it_big_add_overflow | ( | pkc_regs_t * | PKCx | ) |

Disable the big integer overflow interrupt.

Register | BitsName
--- | ---
INTEN | BAOVF

Parameters

  PKCx | PKC instance

Return values

  none. |

## ◆ ll_pkc_disable_it_done()

__STATIC_INLINE void ll_pkc_disable_it_done | ( | pkc_regs_t * | PKCx | ) |

Disable the operation done interrupt.

Register | BitsName
--- | ---
INTEN | DONE

Parameters

  PKCx | PKC instance

Return values

  none. |

## ◆ ll_pkc_disable_it_err()

__STATIC_INLINE void ll_pkc_disable_it_err | ( | pkc_regs_t * | PKCx | ) |

Disable the operation error interrupt.

Register | BitsName
--- | ---
INTEN | ERR

Parameters

  PKCx | PKC instance

Return values

  none. |

## ◆ ll_pkc_enable_it_big_add_overflow()

__STATIC_INLINE void ll_pkc_enable_it_big_add_overflow | ( | pkc_regs_t * | PKCx | ) |

Enable the big integer overflow interrupt.

Register | BitsName
--- | ---
INTEN | BAOVF

Parameters

  PKCx | PKC instance

Return values

  none. |

## ◆ ll_pkc_enable_it_done()

__STATIC_INLINE void ll_pkc_enable_it_done | ( | pkc_regs_t * | PKCx | ) |

Enable the operation done interrupt.

Register | BitsName
--- | ---
INTEN | DONE

Parameters

  PKCx | PKC instance

Return values

  none. |

## ◆ ll_pkc_enable_it_err()

__STATIC_INLINE void ll_pkc_enable_it_err | ( | pkc_regs_t * | PKCx | ) |

Enable the operation error interrupt.

Register | BitsName
--- | ---
INTEN | ERR

Parameters

  PKCx | PKC instance

Return values

  none. |

## ◆ ll_pkc_is_enable_it_big_add_overflow()

__STATIC_INLINE uint32_t ll_pkc_is_enable_it_big_add_overflow | ( | pkc_regs_t * | PKCx | ) |

Indicate whether the big integer overflow interrupt is enable.

Register | BitsName
--- | ---
INTEN | BAOVF

Parameters

  PKCx | PKC instance

Return values

  State | of bit (1 or 0).

## ◆ ll_pkc_is_enable_it_done()

__STATIC_INLINE uint32_t ll_pkc_is_enable_it_done | ( | pkc_regs_t * | PKCx | ) |

Indicate whether the operation done interrupt is enable.

Register | BitsName
--- | ---
INTEN | DONE

Parameters

  PKCx | PKC instance

Return values

  State | of bit (1 or 0).

## ◆ ll_pkc_is_enable_it_err()

__STATIC_INLINE uint32_t ll_pkc_is_enable_it_err | ( | pkc_regs_t * | PKCx | ) |

Indicate whether the operation error interrupt is enable.

Register | BitsName
--- | ---
INTEN | ERR

Parameters

  PKCx | PKC instance

Return values

  State | of bit (1 or 0).