Data Fields
ths_c_handles_t Struct Reference
BLE Services » Throughput Service Client (THS_C) » Structures

Handles on the connected peer device needed to interact with it. More...

`#include <ths_c.h>`

## Data Fields
uint16_t | ths_srvc_start_handle
uint16_t | ths_srvc_end_handle
uint16_t | ths_tx_handle
uint16_t | ths_tx_cccd_handle
uint16_t | ths_rx_handle
uint16_t | ths_setting_handle
uint16_t | ths_setting_cccd_handle
uint16_t | ths_toggle_handle

## Detailed Description

Handles on the connected peer device needed to interact with it.

## Field Documentation

## ◆ ths_rx_handle

uint16_t ths_c_handles_t::ths_rx_handle

THS Rx characteristic handle which has been got from peer.

## ◆ ths_setting_cccd_handle

uint16_t ths_c_handles_t::ths_setting_cccd_handle

THS setting characteristic CCCD handle which has been got from peer.

## ◆ ths_setting_handle

uint16_t ths_c_handles_t::ths_setting_handle

THS setting characteristic handle which has been got from peer.

## ◆ ths_srvc_end_handle

uint16_t ths_c_handles_t::ths_srvc_end_handle

THS Service end handle.

## ◆ ths_srvc_start_handle

uint16_t ths_c_handles_t::ths_srvc_start_handle

THS Service start handle.

## ◆ ths_toggle_handle

uint16_t ths_c_handles_t::ths_toggle_handle

THS toggle characteristic handle which has been got from peer.

## ◆ ths_tx_cccd_handle

uint16_t ths_c_handles_t::ths_tx_cccd_handle

THS Tx characteristic CCCD handle which has been got from peer.

## ◆ ths_tx_handle

uint16_t ths_c_handles_t::ths_tx_handle

THS Tx characteristic handle which has been got from peer.

The documentation for this struct was generated from the following file:

- ths_c.h