Data Fields
ble_gattc_ntf_ind_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Client » Structures

GATTC Notification and Indication value indication. More...

`#include <ble_gattc.h>`

## Data Fields
gatt_evt_type_t | type
uint16_t | length
uint16_t | handle
uint8_t * | p_value

## Detailed Description

GATTC Notification and Indication value indication.

## Field Documentation

## ◆ handle

uint16_t ble_gattc_ntf_ind_t::handle

Attribute handle.

## ◆ length

uint16_t ble_gattc_ntf_ind_t::length

Attribute value length.

## ◆ p_value

uint8_t* ble_gattc_ntf_ind_t::p_value

Pointer to the attribute value data.

## ◆ type

gatt_evt_type_t ble_gattc_ntf_ind_t::type

Event type.

The documentation for this struct was generated from the following file:

- ble_gattc.h