Data Fields
gattc_write_attr_value_t Struct Reference
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Client » Structures

GATTC write attribute value structure. More...

`#include <ble_gattc.h>`

## Data Fields
uint16_t | handle
uint16_t | offset
uint16_t | length
uint8_t * | p_value

## Detailed Description

GATTC write attribute value structure.

## Field Documentation

## ◆ handle

uint16_t gattc_write_attr_value_t::handle

Attribute handle.

## ◆ length

uint16_t gattc_write_attr_value_t::length

Write length.

## ◆ offset

uint16_t gattc_write_attr_value_t::offset

value offset to start with.

## ◆ p_value

uint8_t* gattc_write_attr_value_t::p_value

Value to write.

The documentation for this struct was generated from the following file:

- ble_gattc.h