Modules | Macros
Defines
SYSTEM » Device Firmware Update

## Modules
| DFU cmd disable option (bitmask)

## Macros
#define | DFU_ADV_MAX_LENGTH 18
| The max length of advertisement is 18 bytes. More...
#define | RECEIVE_MAX_LEN 2048
| The max length of received data is 2048 bytes. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DFU_ADV_MAX_LENGTH

#define DFU_ADV_MAX_LENGTH 18

The max length of advertisement is 18 bytes.

Definition at line 56 of file gr55xx_dfu.h.

## ◆ RECEIVE_MAX_LEN

#define RECEIVE_MAX_LEN 2048

The max length of received data is 2048 bytes.

Definition at line 57 of file gr55xx_dfu.h.