Macros
FIFO Threshold
Peripheral Driver » LL Driver » I2S » Defines » I2S Exported Constants

## Macros
#define | LL_I2S_THRESHOLD_1FIFO (0x00000000UL)
| Trigger level for FIFO: 1 depth. More...
#define | LL_I2S_THRESHOLD_2FIFO (1UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 2 depth. More...
#define | LL_I2S_THRESHOLD_3FIFO (2UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 3 depth. More...
#define | LL_I2S_THRESHOLD_4FIFO (3UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 4 depth. More...
#define | LL_I2S_THRESHOLD_5FIFO (4UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 5 depth. More...
#define | LL_I2S_THRESHOLD_6FIFO (5UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 6 depth. More...
#define | LL_I2S_THRESHOLD_7FIFO (6UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 7 depth. More...
#define | LL_I2S_THRESHOLD_8FIFO (7UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 8 depth. More...
#define | LL_I2S_THRESHOLD_9FIFO (8UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 9 depth. More...
#define | LL_I2S_THRESHOLD_10FIFO (9UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 10 depth. More...
#define | LL_I2S_THRESHOLD_11FIFO (10UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 11 depth. More...
#define | LL_I2S_THRESHOLD_12FIFO (11UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 12 depth. More...
#define | LL_I2S_THRESHOLD_13FIFO (12UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 13 depth. More...
#define | LL_I2S_THRESHOLD_14FIFO (13UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 14 depth. More...
#define | LL_I2S_THRESHOLD_15FIFO (14UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 15 depth. More...
#define | LL_I2S_THRESHOLD_16FIFO (15UL << I2S_RXFIFO_TL_Pos)
| Trigger level for FIFO: 16 depth. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2S_THRESHOLD_10FIFO

#define LL_I2S_THRESHOLD_10FIFO (9UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 10 depth.

Definition at line 181 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_11FIFO

#define LL_I2S_THRESHOLD_11FIFO (10UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 11 depth.

Definition at line 182 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_12FIFO

#define LL_I2S_THRESHOLD_12FIFO (11UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 12 depth.

Definition at line 183 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_13FIFO

#define LL_I2S_THRESHOLD_13FIFO (12UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 13 depth.

Definition at line 184 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_14FIFO

#define LL_I2S_THRESHOLD_14FIFO (13UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 14 depth.

Definition at line 185 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_15FIFO

#define LL_I2S_THRESHOLD_15FIFO (14UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 15 depth.

Definition at line 186 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_16FIFO

#define LL_I2S_THRESHOLD_16FIFO (15UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 16 depth.

Definition at line 187 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_1FIFO

#define LL_I2S_THRESHOLD_1FIFO (0x00000000UL)

Trigger level for FIFO: 1 depth.

Definition at line 172 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_2FIFO

#define LL_I2S_THRESHOLD_2FIFO (1UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 2 depth.

Definition at line 173 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_3FIFO

#define LL_I2S_THRESHOLD_3FIFO (2UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 3 depth.

Definition at line 174 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_4FIFO

#define LL_I2S_THRESHOLD_4FIFO (3UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 4 depth.

Definition at line 175 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_5FIFO

#define LL_I2S_THRESHOLD_5FIFO (4UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 5 depth.

Definition at line 176 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_6FIFO

#define LL_I2S_THRESHOLD_6FIFO (5UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 6 depth.

Definition at line 177 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_7FIFO

#define LL_I2S_THRESHOLD_7FIFO (6UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 7 depth.

Definition at line 178 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_8FIFO

#define LL_I2S_THRESHOLD_8FIFO (7UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 8 depth.

Definition at line 179 of file gr55xx_ll_i2s.h.

## ◆ LL_I2S_THRESHOLD_9FIFO

#define LL_I2S_THRESHOLD_9FIFO (8UL << I2S_RXFIFO_TL_Pos)

Trigger level for FIFO: 9 depth.

Definition at line 180 of file gr55xx_ll_i2s.h.