Macros
Power States Defines
Peripheral Driver » HAL Driver » ISO7816 » Defines » ISO7816 Exported Constants

## Macros
#define | HAL_ISO7816_PWR_STATE_OFF LL_ISO7816_PWR_STATE_OFF
| Off More...
#define | HAL_ISO7816_PWR_STATE_PWRUP_VCC LL_ISO7816_PWR_STATE_PWRUP_VCC
| Power up VCC More...
#define | HAL_ISO7816_PWR_STATE_PWRUP_RST LL_ISO7816_PWR_STATE_PWRUP_RST
| Power up reset More...
#define | HAL_ISO7816_PWR_STATE_PWRDN_RST LL_ISO7816_PWR_STATE_PWRDN_RST
| Power Down reset More...
#define | HAL_ISO7816_PWR_STATE_PWRDN_VCC LL_ISO7816_PWR_STATE_PWRDN_VCC
| Power Down VCC More...
#define | HAL_ISO7816_PWR_STATE_STOP_PRE LL_ISO7816_PWR_STATE_STOP_PRE
| Preparing Clock Stop More...
#define | HAL_ISO7816_PWR_STATE_STOP LL_ISO7816_PWR_STATE_STOP
| Clock Stopped More...
#define | HAL_ISO7816_PWR_STATE_STOP_POST LL_ISO7816_PWR_STATE_STOP_POST
| Exiting Clock Stop More...
#define | HAL_ISO7816_PWR_STATE_IDLE LL_ISO7816_PWR_STATE_IDLE
| Idle More...
#define | HAL_ISO7816_PWR_STATE_RX_TS0 LL_ISO7816_PWR_STATE_RX_TS0
| RX TS Character More...
#define | HAL_ISO7816_PWR_STATE_RX_TS1 LL_ISO7816_PWR_STATE_RX_TS1
| RX TS Character More...
#define | HAL_ISO7816_PWR_STATE_RX LL_ISO7816_PWR_STATE_RX
| Receive More...
#define | HAL_ISO7816_PWR_STATE_TX LL_ISO7816_PWR_STATE_TX
| Transmit More...
#define | HAL_ISO7816_PWR_STATE_TX_RX LL_ISO7816_PWR_STATE_TX_RX
| Transmit and Receive More...

## Detailed Description

## Macro Definition Documentation

## ◆ HAL_ISO7816_PWR_STATE_IDLE

#define HAL_ISO7816_PWR_STATE_IDLE LL_ISO7816_PWR_STATE_IDLE

Idle

Definition at line 252 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_OFF

#define HAL_ISO7816_PWR_STATE_OFF LL_ISO7816_PWR_STATE_OFF

Off

Definition at line 244 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRDN_RST

#define HAL_ISO7816_PWR_STATE_PWRDN_RST LL_ISO7816_PWR_STATE_PWRDN_RST

Power Down reset

Definition at line 247 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRDN_VCC

#define HAL_ISO7816_PWR_STATE_PWRDN_VCC LL_ISO7816_PWR_STATE_PWRDN_VCC

Power Down VCC

Definition at line 248 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRUP_RST

#define HAL_ISO7816_PWR_STATE_PWRUP_RST LL_ISO7816_PWR_STATE_PWRUP_RST

Power up reset

Definition at line 246 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_PWRUP_VCC

#define HAL_ISO7816_PWR_STATE_PWRUP_VCC LL_ISO7816_PWR_STATE_PWRUP_VCC

Power up VCC

Definition at line 245 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_RX

#define HAL_ISO7816_PWR_STATE_RX LL_ISO7816_PWR_STATE_RX

Receive

Definition at line 255 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_RX_TS0

#define HAL_ISO7816_PWR_STATE_RX_TS0 LL_ISO7816_PWR_STATE_RX_TS0

RX TS Character

Definition at line 253 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_RX_TS1

#define HAL_ISO7816_PWR_STATE_RX_TS1 LL_ISO7816_PWR_STATE_RX_TS1

RX TS Character

Definition at line 254 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_STOP

#define HAL_ISO7816_PWR_STATE_STOP LL_ISO7816_PWR_STATE_STOP

Clock Stopped

Definition at line 250 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_STOP_POST

#define HAL_ISO7816_PWR_STATE_STOP_POST LL_ISO7816_PWR_STATE_STOP_POST

Exiting Clock Stop

Definition at line 251 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_STOP_PRE

#define HAL_ISO7816_PWR_STATE_STOP_PRE LL_ISO7816_PWR_STATE_STOP_PRE

Preparing Clock Stop

Definition at line 249 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_TX

#define HAL_ISO7816_PWR_STATE_TX LL_ISO7816_PWR_STATE_TX

Transmit

Definition at line 256 of file gr55xx_hal_iso7816.h.

## ◆ HAL_ISO7816_PWR_STATE_TX_RX

#define HAL_ISO7816_PWR_STATE_TX_RX LL_ISO7816_PWR_STATE_TX_RX

Transmit and Receive

Definition at line 257 of file gr55xx_hal_iso7816.h.