Macros
External Wakeup Control Low Significant Bit Defines
Peripheral Driver » LL Driver » PWR » Defines » PWR Private Constants

## Macros
#define | LL_PWR_EXTWKUP_TYPE_LSB (0x01U << AON_EXT_WKUP_CTL_TYPE_Pos)
| External wakeup level type. More...
#define | LL_PWR_EXTWKUP_INVERT_LSB (0x01U << AON_EXT_WKUP_CTL_INVERT_Pos)
| External wakeup level invert. More...
#define | LL_PWR_EXTWKUP_SRC_EN_LSB (0x01U << AON_EXT_WKUP_CTL_SRC_EN_Pos)
| External wakeup source enable. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_PWR_EXTWKUP_INVERT_LSB

#define LL_PWR_EXTWKUP_INVERT_LSB (0x01U << AON_EXT_WKUP_CTL_INVERT_Pos)

External wakeup level invert.

Definition at line 80 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_SRC_EN_LSB

#define LL_PWR_EXTWKUP_SRC_EN_LSB (0x01U << AON_EXT_WKUP_CTL_SRC_EN_Pos)

External wakeup source enable.

Definition at line 81 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_TYPE_LSB

#define LL_PWR_EXTWKUP_TYPE_LSB (0x01U << AON_EXT_WKUP_CTL_TYPE_Pos)

External wakeup level type.

Definition at line 79 of file gr55xx_ll_pwr.h.