Macros
Own Address Length
Peripheral Driver » LL Driver » I2C » Defines » I2C Exported Constants

## Macros
#define | LL_I2C_OWNADDRESS_7BIT 0x00000000U
| Own address 1 is a 7-bit address. More...
#define | LL_I2C_OWNADDRESS_10BIT I2C_CON_10BITADDR_SLV
| Own address 1 is a 10-bit address. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_I2C_OWNADDRESS_10BIT

#define LL_I2C_OWNADDRESS_10BIT I2C_CON_10BITADDR_SLV

Own address 1 is a 10-bit address.

Definition at line 177 of file gr55xx_ll_i2c.h.

## ◆ LL_I2C_OWNADDRESS_7BIT

#define LL_I2C_OWNADDRESS_7BIT 0x00000000U

Own address 1 is a 7-bit address.

Definition at line 176 of file gr55xx_ll_i2c.h.