Macros
Advertising type
BLE Services » Alexa Gadget Service (AGS) » Defines

The advertisiment type. More...

## Macros
#define | AGS_PAIR_ADV_FLAG 0x01
| The Pairing advertisiment flag. More...
#define | AGS_RECONNECT_ADV_FLAG 0x00
| The reconnecting advertisiment flag. More...

## Detailed Description

The advertisiment type.

Bit 0 : Pairing or reconnection mode, 0 - reconnection mode, 1 - pairing mode; Bit 1 : Classic Bluetooth discoverability; Bit 2~7 : Reserved for future use, set to 0x00.

## Macro Definition Documentation

## ◆ AGS_PAIR_ADV_FLAG

#define AGS_PAIR_ADV_FLAG 0x01

The Pairing advertisiment flag.

Definition at line 89 of file ags.h.

## ◆ AGS_RECONNECT_ADV_FLAG

#define AGS_RECONNECT_ADV_FLAG 0x00

The reconnecting advertisiment flag.

Definition at line 90 of file ags.h.