Macros
DUAL TIMER Prescaler Division
Peripheral Driver » HAL Driver » DUAL TIMER » Defines » DUAL TIMER Exported Constants

## Macros
#define | DUAL_TIMER_PRESCALER_DIV0 LL_DUAL_TIMER_PRESCALER_DIV0
| 0 stage of prescale, clock is divided by 1. More...
#define | DUAL_TIMER_PRESCALER_DIV16 LL_DUAL_TIMER_PRESCALER_DIV16
| 4 stages of prescale, clock is divided by 16. More...
#define | DUAL_TIMER_PRESCALER_DIV256 LL_DUAL_TIMER_PRESCALER_DIV256
| 8 stages of prescale, clock is divided by 256. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DUAL_TIMER_PRESCALER_DIV0

#define DUAL_TIMER_PRESCALER_DIV0 LL_DUAL_TIMER_PRESCALER_DIV0

0 stage of prescale, clock is divided by 1.

Definition at line 168 of file gr55xx_hal_dual_tim.h.

## ◆ DUAL_TIMER_PRESCALER_DIV16

#define DUAL_TIMER_PRESCALER_DIV16 LL_DUAL_TIMER_PRESCALER_DIV16

4 stages of prescale, clock is divided by 16.

Definition at line 169 of file gr55xx_hal_dual_tim.h.

## ◆ DUAL_TIMER_PRESCALER_DIV256

#define DUAL_TIMER_PRESCALER_DIV256 LL_DUAL_TIMER_PRESCALER_DIV256

8 stages of prescale, clock is divided by 256.

Definition at line 170 of file gr55xx_hal_dual_tim.h.