Functions
Data Management
Peripheral Driver » LL Driver » RNG » Functions

## Functions
__STATIC_INLINE uint32_t | ll_rng_read_random_data32 (rng_regs_t *RNGx)
| Return32-bit Random Number value. More...
__STATIC_INLINE uint32_t | ll_rng_read_lr_count (rng_regs_t *RNGx)
| Return8-bit RNG Long Run Test counts. More...

## Detailed Description

## Function Documentation

## ◆ ll_rng_read_lr_count()

__STATIC_INLINE uint32_t ll_rng_read_lr_count | ( | rng_regs_t * | RNGx | ) |

Return8-bit RNG Long Run Test counts.

Register | BitsName
--- | ---
LR_STATUS | RNG_LR_CNT

Parameters

  RNGx | RNG instance.

Return values

  Output | Data[7:0]

Definition at line 611 of file gr55xx_ll_rng.h.

## ◆ ll_rng_read_random_data32()

__STATIC_INLINE uint32_t ll_rng_read_random_data32 | ( | rng_regs_t * | RNGx | ) |

Return32-bit Random Number value.

Register | BitsName
--- | ---
DATA | RNG_DATA

Parameters

  RNGx | RNG instance.

Return values

  Generated | 32-bit random value

Definition at line 596 of file gr55xx_ll_rng.h.