Classes
Structures
BLE » Generic Access Profile (GAP) » Generic Access Profile (GAP) Connection Control
Collaboration diagram for Structures:

## Classes
struct | ble_gap_dev_version_ind_t
| The struct of device version. More...
struct | ble_gap_addr_t
| The struct of address. More...
struct | ble_gap_bdaddr_t
| The struct of broadcast address with broadcast type. More...
struct | ble_gap_get_bd_addr_t
| Get broadcast address struct. More...
struct | ble_gap_dev_adv_tx_power_t
| TX power info struct. More...
struct | ble_gap_dev_tx_power_t
| TX power info struct. More...
struct | ble_gap_max_data_len_t
| Max data length info struct. More...
struct | ble_gap_sugg_dflt_data_len_t
| Suggested default data length info. More...
struct | ble_gap_nb_adv_sets_t
| Number of available advertising sets info. More...
struct | ble_gap_max_adv_data_len_ind_t
| Maximum advertising data length info. More...
struct | ble_gap_dev_rf_path_comp_ind_t
| RF path compensation values info. More...
union | ble_gap_dev_info_t
| Device info. More...
struct | ble_gap_conn_param_t
| The parameter of connection. More...
struct | ble_gap_conn_update_param_t
| The parameter of update connection. More...
struct | ble_gap_chnl_map_t
| Channel map structure. More...
struct | ble_gap_le_phy_ind_t
| PHY info. More...
union | ble_gap_conn_info_t
| Connection info. More...
struct | ble_gap_peer_version_ind_t
| Peer version info. More...
struct | ble_gap_peer_features_ind_t
| LE features info. More...
union | ble_gap_peer_info_t
| LE peer info. More...
struct | ble_gap_con_plan_tag_t
| The Structure for BLE Connection Arrangement. More...
struct | ble_gap_set_pref_slave_evt_dur_param_t
| Set preference slave event duration. More...
struct | ble_gap_evt_phy_update_t
| PHY update event for BLE_GAPC_EVT_PHY_UPDATED. More...
struct | ble_gap_evt_dev_info_get_t
| Get device info event for BLE_GAPC_EVT_DEV_INFO_GOT. More...
struct | ble_gap_evt_connected_t
| Connection complete event for BLE_GAPC_EVT_CONNECTED. More...
struct | ble_gap_evt_disconnected_t
| Disconnection event for BLE_GAPC_EVT_DISCONNECTED. More...
struct | ble_gap_evt_peer_name_get_t
| Name of peer device indication event for BLE_GAPC_EVT_PEER_NAME_GOT. More...
struct | ble_gap_evt_peer_info_t
| Get peer info event for BLE_GAPC_EVT_PEER_INFO_GOT. More...
struct | ble_gap_evt_conn_param_updated_t
| Connection parameter updated event for BLE_GAPC_EVT_CONN_PARAM_UPDATED. More...
struct | ble_gap_evt_conn_param_update_req_t
| Connection parameter update request event for BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ. More...
struct | ble_gap_evt_conn_info_t
| Get Connection info event for BLE_GAPC_EVT_CONN_INFO_GOT. More...
struct | ble_gap_evt_data_length_t
| Data Length Updated event for BLE_GAPC_EVT_DATA_LENGTH_UPDATED. More...
struct | ble_gapc_evt_t
| BLE GAPC event structure. More...

## Detailed Description