Public Attributes | List of all members
ble_sec_param_t Struct Reference
BLE » Security Manager(SM) » Structures

SEC Parameter. More...

`#include <ble_sec.h>`

## Public Attributes
ble_sec_mode_level_t | level
| Set the minimum security level of the device, see ble_sec_mode_level_t. More...
ble_sec_io_cap_t | io_cap
| Set the IO capability, see ble_sec_io_cap_t. More...
bool | oob
| Indicate whether OOB is supported. More...
uint8_t | auth
| Set the auth, see SEC Auth Flag. More...
uint8_t | key_size
| Indicate the supported maximum LTK size (range: 7-16). More...
uint8_t | ikey_dist
| Set the initial key distribution, see SEC Key Distribution Flag. More...
uint8_t | rkey_dist
| Set the response key distribution, see SEC Key Distribution Flag. More...

## Detailed Description

SEC Parameter.

Definition at line 147 of file ble_sec.h.

## Member Data Documentation

## ◆ auth

uint8_t ble_sec_param_t::auth

Set the auth, see SEC Auth Flag.

Definition at line 152 of file ble_sec.h.

## ◆ ikey_dist

uint8_t ble_sec_param_t::ikey_dist

Set the initial key distribution, see SEC Key Distribution Flag.

Definition at line 154 of file ble_sec.h.

## ◆ io_cap

ble_sec_io_cap_t ble_sec_param_t::io_cap

Set the IO capability, see ble_sec_io_cap_t.

Definition at line 150 of file ble_sec.h.

## ◆ key_size

uint8_t ble_sec_param_t::key_size

Indicate the supported maximum LTK size (range: 7-16).

Definition at line 153 of file ble_sec.h.

## ◆ level

ble_sec_mode_level_t ble_sec_param_t::level

Set the minimum security level of the device, see ble_sec_mode_level_t.

Definition at line 149 of file ble_sec.h.

## ◆ oob

bool ble_sec_param_t::oob

Indicate whether OOB is supported.

Definition at line 151 of file ble_sec.h.

## ◆ rkey_dist

uint8_t ble_sec_param_t::rkey_dist

Set the response key distribution, see SEC Key Distribution Flag.

Definition at line 155 of file ble_sec.h.

The documentation for this struct was generated from the following file:

- ble_sec.h