Macros
External Wakeup Pins
Peripheral Driver » LL Driver » PWR » Defines » PWR Exported Constants
Collaboration diagram for External Wakeup Pins:

## Macros
#define | LL_PWR_EXTWKUP_PIN0 (0x00000001U)
| WKUP pin 0 : AON_GPIO_PIN0. More...
#define | LL_PWR_EXTWKUP_PIN1 (0x00000002U)
| WKUP pin 1 : AON_GPIO_PIN1. More...
#define | LL_PWR_EXTWKUP_PIN2 (0x00000004U)
| WKUP pin 2 : AON_GPIO_PIN2. More...
#define | LL_PWR_EXTWKUP_PIN3 (0x00000008U)
| WKUP pin 3 : AON_GPIO_PIN3. More...
#define | LL_PWR_EXTWKUP_PIN4 (0x00000010U)
| WKUP pin 4 : AON_GPIO_PIN4. More...
#define | LL_PWR_EXTWKUP_PIN5 (0x00000020U)
| WKUP pin 5 : AON_GPIO_PIN5. More...
#define | LL_PWR_EXTWKUP_PIN6 (0x00000040U)
| WKUP pin 6 : AON_GPIO_PIN6. More...
#define | LL_PWR_EXTWKUP_PIN7 (0x00000080U)
| WKUP pin 7 : AON_GPIO_PIN7. More...
#define | LL_PWR_EXTWKUP_PIN_ALL (0x000000FFU)
| WKUP pin all : AON_GPIO_PIN0 ~ AON_GPIO_PIN7. More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_PWR_EXTWKUP_PIN0

#define LL_PWR_EXTWKUP_PIN0 (0x00000001U)

WKUP pin 0 : AON_GPIO_PIN0.

Definition at line 147 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN1

#define LL_PWR_EXTWKUP_PIN1 (0x00000002U)

WKUP pin 1 : AON_GPIO_PIN1.

Definition at line 148 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN2

#define LL_PWR_EXTWKUP_PIN2 (0x00000004U)

WKUP pin 2 : AON_GPIO_PIN2.

Definition at line 149 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN3

#define LL_PWR_EXTWKUP_PIN3 (0x00000008U)

WKUP pin 3 : AON_GPIO_PIN3.

Definition at line 150 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN4

#define LL_PWR_EXTWKUP_PIN4 (0x00000010U)

WKUP pin 4 : AON_GPIO_PIN4.

Definition at line 151 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN5

#define LL_PWR_EXTWKUP_PIN5 (0x00000020U)

WKUP pin 5 : AON_GPIO_PIN5.

Definition at line 152 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN6

#define LL_PWR_EXTWKUP_PIN6 (0x00000040U)

WKUP pin 6 : AON_GPIO_PIN6.

Definition at line 153 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN7

#define LL_PWR_EXTWKUP_PIN7 (0x00000080U)

WKUP pin 7 : AON_GPIO_PIN7.

Definition at line 154 of file gr55xx_ll_pwr.h.

## ◆ LL_PWR_EXTWKUP_PIN_ALL

#define LL_PWR_EXTWKUP_PIN_ALL (0x000000FFU)

WKUP pin all : AON_GPIO_PIN0 ~ AON_GPIO_PIN7.

Definition at line 155 of file gr55xx_ll_pwr.h.