Functions
IT_Management
Peripheral Driver » LL Driver » TIMER » Functions
Collaboration diagram for IT_Management:

## Functions
__STATIC_INLINE void | ll_timer_enable_it (timer_regs_t *TIMERx)
| Enable timer interrupt. More...
__STATIC_INLINE void | ll_timer_disable_it (timer_regs_t *TIMERx)
| Disable timer interrput. More...
__STATIC_INLINE uint32_t | ll_timer_is_enabled_it (timer_regs_t *TIMERx)
| Indicate whether the timer interrput is enabled. More...

## Detailed Description

## Function Documentation

## ◆ ll_timer_disable_it()

__STATIC_INLINE void ll_timer_disable_it | ( | timer_regs_t * | TIMERx | ) |

Disable timer interrput.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | CTRL | INTEN | +-------------------—+--------------------------------—+ \endrst

Parameters

  TIMERx | Timer instance

Return values

  None |

Definition at line 329 of file gr55xx_ll_tim.h.

## ◆ ll_timer_enable_it()

__STATIC_INLINE void ll_timer_enable_it | ( | timer_regs_t * | TIMERx | ) |

Enable timer interrupt.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | CTRL | INTEN | +-------------------—+--------------------------------—+ \endrst

Parameters

  TIMERx | Timer instance

Return values

  None |

Definition at line 310 of file gr55xx_ll_tim.h.

## ◆ ll_timer_is_enabled_it()

__STATIC_INLINE uint32_t ll_timer_is_enabled_it | ( | timer_regs_t * | TIMERx | ) |

Indicate whether the timer interrput is enabled.

\rst +-------------------—+--------------------------------—+ | Register | BitsName | +======================+===================================+ | CTRL | INTEN | +-------------------—+--------------------------------—+ \endrst

Parameters

  TIMERx | Timer instance

Return values

  State | of bit (1 or 0).

Definition at line 348 of file gr55xx_ll_tim.h.