ble_event.h
Go to the documentation of this file.
1 /**
2 ****************************************************************************************
3 *
4 * @file ble_event.h
5 *
6 * @brief BLE event header files
7 *
8 ****************************************************************************************
9 * @attention
10 #####Copyright (c) 2019 GOODIX
11 All rights reserved.
12
13 Redistribution and use in source and binary forms, with or without
14 modification, are permitted provided that the following conditions are met:
15 * Redistributions of source code must retain the above copyright
16 notice, this list of conditions and the following disclaimer.
17 * Redistributions in binary form must reproduce the above copyright
18 notice, this list of conditions and the following disclaimer in the
19 documentation and/or other materials provided with the distribution.
20 * Neither the name of GOODIX nor the names of its contributors may be used
21 to endorse or promote products derived from this software without
22 specific prior written permission.
23
24 THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
25 AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
26 IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE
27 ARE DISCLAIMED. IN NO EVENT SHALL COPYRIGHT HOLDERS AND CONTRIBUTORS BE
28 LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
29 CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF
30 SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS
31 INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
32 CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
33 ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
34 POSSIBILITY OF SUCH DAMAGE.
35 *****************************************************************************************
36 */
37
38 /**
39 * @addtogroup BLE
40 * @{
41 */
42
43 /**
44 @addtogroup BLE_EVENT BLE Event
45 @{
46 @brief BLE Event interface.
47 */
48 #ifndef __BLE_EVENT_H__
49 #define __BLE_EVENT_H__
50
51 #include "ble_gapm.h"
52 #include "ble_gapc.h"
53 #include "ble_gatts.h"
54 #include "ble_gattc.h"
55 #include "ble_sec.h"
56 #include "ble_l2cap.h"
57
58 /** @addtogroup BLE_EVENT_DEFINES Defines
59 * @{
60 */
61 /** @defgroup BLE_EVENT_BASE BLE Event Base
62 * @{ */
63 #define BLE_COMMON_EVT_BASE 0x0100 /**< BLE Common Event base. */
64 #define BLE_GAPM_EVT_BASE 0x0200 /**< BLE GAP Management Event base. */
65 #define BLE_GAPC_EVT_BASE 0x0300 /**< BLE GAP Connection Control Event base. */
66 #define BLE_GATTS_EVT_BASE 0x0400 /**< BLE GATTS Event base. */
67 #define BLE_GATTC_EVT_BASE 0x0500 /**< BLE GATTC Event base. */
68 #define BLE_GATT_COMMON_EVT_BASE 0x0600 /**< BLE GATT Event base. */
69 #define BLE_SEC_EVT_BASE 0x0700 /**< BLE Security Event base. */
70 #define BLE_L2CAP_EVT_BASE 0x0800 /**< BLE L2CAP Event base. */
71 /** @} */
72 /** @} */
73
74 /**
75 * @defgroup BLE_EVENT_ENUM Enumerations
76 * @{
77 */
78 /**
79 * @brief BLE Common Events.
80 */
81 enum BLE_COMMON_EVTS
82 {
83 BLE_COMMON_EVT_STACK_INIT = BLE_COMMON_EVT_BASE, /**< BLE Stack init complete event. */
84 BLE_COMMON_EVT_MAX,
85 };
86
87 /**@brief BLE GAP Managerment Events. */
88 enum BLE_GAPM_EVTS
89 {
90 BLE_GAPM_EVT_CH_MAP_SET = BLE_GAPM_EVT_BASE, /**< Channel Map Set complete event. */
91 BLE_GAPM_EVT_WHITELIST_SET, /**< Whitelist Set complete event. */
92 BLE_GAPM_EVT_PER_ADV_LIST_SET, /**< Periodic Advertising List Set complete event. */
93 BLE_GAPM_EVT_PRIVACY_MODE_SET, /**< Privacy Mode for Peer Device Set complete event. */
94 BLE_GAPM_EVT_LEPSM_REGISTER, /**< LEPSM Register complete event. */
95 BLE_GAPM_EVT_LEPSM_UNREGISTER, /**< LEPSM Unregister complete event. */
96 BLE_GAPM_EVT_DEV_INFO_GOT, /**< Device Info Get event. */
97 BLE_GAPM_EVT_ADV_START, /**< Advertising Start complete event. */
98 BLE_GAPM_EVT_ADV_STOP, /**< Advertising Stop complete event. */
99 BLE_GAPM_EVT_SCAN_REQUEST, /**< Scan Request event. */
100 BLE_GAPM_EVT_ADV_DATA_UPDATE, /**< Advertising Data update event. */
101 BLE_GAPM_EVT_SCAN_START, /**< Scan Start complete event. */
102 BLE_GAPM_EVT_SCAN_STOP, /**< Scan Stop complete event. */
103 BLE_GAPM_EVT_ADV_REPORT, /**< Advertising Report event. */
104 BLE_GAPM_EVT_SYNC_ESTABLISH, /**< Periodic Advertising Synchronization Establish event. */
105 BLE_GAPM_EVT_SYNC_STOP, /**< Periodic Advertising Synchronization Stop event. */
106 BLE_GAPM_EVT_SYNC_LOST, /**< Periodic Advertising Synchronization Lost event. */
107 BLE_GAPM_EVT_READ_RSLV_ADDR, /**< Read Resolvable Address event. */
108 BLE_GAPM_EVT_RSLV_ADDR_REPORT, /**< Resolvable Address report event. */
109 BLE_GAPM_EVT_MAX,
110 };
111
112 /**@brief BLE GAP Connection Control Events. */
113 enum BLE_GAPC_EVTS
114 {
115 BLE_GAPC_EVT_PHY_UPDATED = BLE_GAPC_EVT_BASE, /**< PHY Update event. */
116 BLE_GAPC_EVT_CONNECTED, /**< Connected event. */
117 BLE_GAPC_EVT_DISCONNECTED, /**< Disconnected event. */
118 BLE_GAPC_EVT_CONNECT_CANCLE, /**< Connect Cancle event. */
119 BLE_GAPC_EVT_AUTO_CONN_TIMEOUT, /**< Auto Connect Timeout event. */
120 BLE_GAPC_EVT_CONN_PARAM_UPDATED, /**< Connect Parameter Updated event. */
121 BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ, /**< Connect Parameter Request event. */
122 BLE_GAPC_EVT_PEER_NAME_GOT, /**< peer Name Get event. */
123 BLE_GAPC_EVT_CONN_INFO_GOT, /**< Connect Info Get event. */
124 BLE_GAPC_EVT_PEER_INFO_GOT, /**< Peer Info Get event. */
125 BLE_GAPC_EVT_DATA_LENGTH_UPDATED, /**< Data Length Updated event. */
126 BLE_GAPC_EVT_MAX,
127 };
128
129 /**@brief BLE GATT Common Events. */
130 enum BLE_GATT_COMMON_EVTS
131 {
132 BLE_GATT_COMMON_EVT_MTU_EXCHANGE = BLE_GATT_COMMON_EVT_BASE, /**< MTU Exchange event. */
133 BLE_GATT_COMMON_EVT_PRF_REGISTER, /**< Service Register event. */
134 BLE_GATT_COMMON_EVT_MAX,
135 };
136
137 /**@brief BLE GATTS Events. */
138 enum BLE_GATTS_EVTS
139 {
140 BLE_GATTS_EVT_READ_REQUEST = BLE_GATTS_EVT_BASE, /**< GATTS Read Request event .*/
141 BLE_GATTS_EVT_WRITE_REQUEST, /**< GATTS Write Request event .*/
142 BLE_GATTS_EVT_PREP_WRITE_REQUEST, /**< GATTS Prepare Write Request event .*/
143 BLE_GATTS_EVT_NTF_IND, /**< GATTS Notify or Indicate Complete event .*/
144 BLE_GATTS_EVT_CCCD_RECOVERY, /**< GATTS CCCD Recovery event .*/
145 BLE_GATTS_EVT_DATABASE_INITED_IND,
146 BLE_GATTS_EVT_MAX,
147 };
148
149 /**@brief BLE GATTC Events. */
150 enum BLE_GATTC_EVTS
151 {
152 BLE_GATTC_EVT_SRVC_BROWSE = BLE_GATTC_EVT_BASE, /**< GATTC Service Browse event .*/
153 BLE_GATTC_EVT_PRIMARY_SRVC_DISC, /**< GATTC Primary Service Discovery event .*/
154 BLE_GATTC_EVT_INCLUDE_SRVC_DISC, /**< GATTC Include Service Discovery event .*/
155 BLE_GATTC_EVT_CHAR_DISC, /**< GATTC Characteristic Discovery event .*/
156 BLE_GATTC_EVT_CHAR_DESC_DISC, /**< GATTC Characteristic Descriptor Discovery event .*/
157 BLE_GATTC_EVT_READ_RSP, /**< GATTC Read Response event. */
158 BLE_GATTC_EVT_WRITE_RSP, /**< GATTC Write Response event. */
159 BLE_GATTC_EVT_NTF_IND, /**< GATTC Notify or Indicate Receive event. */
160 BLE_GATTC_EVT_MAX,
161 };
162
163 /**@brief BLE SEC Events. */
164 enum BLE_SEC_EVTS
165 {
166 BLE_SEC_EVT_LINK_ENC_REQUEST = BLE_SEC_EVT_BASE, /**< Link Encrypte Request event. */
167 BLE_SEC_EVT_LINK_ENCRYPTED, /**< Link Encrypted event. */
168 BLE_SEC_EVT_LTK_REQ, /**< LTK Request event. */
169 BLE_SEC_EVT_KEY_PRESS_NTF, /**< Key Press event. */
170 BLE_SEC_EVT_KEY_MISSING, /**< Key Missing event. */
171 BLE_SEC_EVT_MAX,
172 };
173
174 /**@brief BLE L2CAP Events. */
175 enum BLE_L2CAP_EVTS
176 {
177 BLE_L2CAP_EVT_CONN_REQ = BLE_L2CAP_EVT_BASE, /**< L2cap Connect Request event. */
178 BLE_L2CAP_EVT_CONN_IND, /**< L2cap Connected Indicate event. */
179 BLE_L2CAP_EVT_ADD_CREDITS_IND, /**< L2cap Credits Add Indicate event. */
180 BLE_L2CAP_EVT_DISCONNECTED, /**< L2cap Disconnected event. */
181 BLE_L2CAP_EVT_SDU_RECV, /**< L2cap SDU Receive event. */
182 BLE_L2CAP_EVT_SDU_SEND, /**< L2cap SDU Send event. */
183 BLE_L2CAP_EVT_ADD_CREDITS_CPLT, /**< L2cap Credits Add Completed event. */
184 BLE_L2CAP_EVT_MAX,
185 };
186 /** @} */
187
188 /** @addtogroup BLE_COMMEN_STRUCTURES Structures
189 * @{
190 */
191 /**@brief BLE Event Information. */
192 typedef struct
193 {
194 uint16_t evt_id; /**< Event ID. */
195 uint16_t evt_status; /**< Event Status. */
196 union
197 {
198 ble_gapm_evt_t gapm_evt; /**< BLE GAP Management Event. */
199 ble_gapc_evt_t gapc_evt; /**< BLE GAP Connection Control Event. */
200 ble_gatts_evt_t gatts_evt; /**< BLE GATT Server Event. */
201 ble_gattc_evt_t gattc_evt; /**< BLE GATT Client Event. */
202 ble_gatt_common_evt_t gatt_common_evt; /**< BLE GATT Common Event. */
203 ble_sec_evt_t sec_evt; /**< BLE Security Event. */
204 ble_l2cap_evt_t l2cap_evt; /**< BLE L2CAP Event. */
205 } evt; /**< BLE Event parameter. */
206 } ble_evt_t;
207 /** @} */
208
209 /** @addtogroup BLE_EVENT_TYPEDEF Typedefs
210 * @{
211 */
212 /**@brief The BLE event handler type. */
213 typedef void (*ble_evt_handler_t)(const ble_evt_t *p_evt);
214 /** @} */
215
216 #endif
217 /** @} */
218 /** @} */
219
220
221
222
BLE_GAPM_EVT_PRIVACY_MODE_SET
@ BLE_GAPM_EVT_PRIVACY_MODE_SET
Privacy Mode for Peer Device Set complete event.
Definition: ble_event.h:93
BLE_GAPM_EVTS
BLE_GAPM_EVTS
BLE GAP Managerment Events.
Definition: ble_event.h:89
BLE_GAPM_EVT_SCAN_REQUEST
@ BLE_GAPM_EVT_SCAN_REQUEST
Scan Request event.
Definition: ble_event.h:99
BLE_GATTC_EVT_READ_RSP
@ BLE_GATTC_EVT_READ_RSP
GATTC Read Response event.
Definition: ble_event.h:157
BLE_GAPM_EVT_ADV_START
@ BLE_GAPM_EVT_ADV_START
Advertising Start complete event.
Definition: ble_event.h:97
BLE_GAPM_EVT_BASE
#define BLE_GAPM_EVT_BASE
BLE GAP Management Event base.
Definition: ble_event.h:64
BLE_GATTC_EVT_MAX
@ BLE_GATTC_EVT_MAX
Definition: ble_event.h:160
BLE_GAPM_EVT_ADV_STOP
@ BLE_GAPM_EVT_ADV_STOP
Advertising Stop complete event.
Definition: ble_event.h:98
BLE_GATTS_EVT_PREP_WRITE_REQUEST
@ BLE_GATTS_EVT_PREP_WRITE_REQUEST
GATTS Prepare Write Request event .
Definition: ble_event.h:142
BLE_SEC_EVT_MAX
@ BLE_SEC_EVT_MAX
Definition: ble_event.h:171
BLE_GAPC_EVT_CONN_INFO_GOT
@ BLE_GAPC_EVT_CONN_INFO_GOT
Connect Info Get event.
Definition: ble_event.h:123
BLE_GATTC_EVT_WRITE_RSP
@ BLE_GATTC_EVT_WRITE_RSP
GATTC Write Response event.
Definition: ble_event.h:158
BLE_GATT_COMMON_EVT_MAX
@ BLE_GATT_COMMON_EVT_MAX
Definition: ble_event.h:134
BLE_SEC_EVT_BASE
#define BLE_SEC_EVT_BASE
BLE Security Event base.
Definition: ble_event.h:69
BLE_GAPM_EVT_ADV_REPORT
@ BLE_GAPM_EVT_ADV_REPORT
Advertising Report event.
Definition: ble_event.h:103
BLE_GAPM_EVT_RSLV_ADDR_REPORT
@ BLE_GAPM_EVT_RSLV_ADDR_REPORT
Resolvable Address report event.
Definition: ble_event.h:108
BLE_GATTC_EVT_NTF_IND
@ BLE_GATTC_EVT_NTF_IND
GATTC Notify or Indicate Receive event.
Definition: ble_event.h:159
ble_evt_t::l2cap_evt
ble_l2cap_evt_t l2cap_evt
BLE L2CAP Event.
Definition: ble_event.h:204
BLE_GAPC_EVT_DISCONNECTED
@ BLE_GAPC_EVT_DISCONNECTED
Disconnected event.
Definition: ble_event.h:117
BLE_GATT_COMMON_EVT_MTU_EXCHANGE
@ BLE_GATT_COMMON_EVT_MTU_EXCHANGE
MTU Exchange event.
Definition: ble_event.h:132
BLE_GATT_COMMON_EVTS
BLE_GATT_COMMON_EVTS
BLE GATT Common Events.
Definition: ble_event.h:131
BLE_L2CAP_EVT_CONN_REQ
@ BLE_L2CAP_EVT_CONN_REQ
L2cap Connect Request event.
Definition: ble_event.h:177
ble_evt_t::evt_status
uint16_t evt_status
Event Status.
Definition: ble_event.h:195
BLE_L2CAP_EVT_BASE
#define BLE_L2CAP_EVT_BASE
BLE L2CAP Event base.
Definition: ble_event.h:70
ble_evt_t::gatts_evt
ble_gatts_evt_t gatts_evt
BLE GATT Server Event.
Definition: ble_event.h:200
ble_gatts.h
BLE GATTS API.
ble_l2cap_evt_t
BLE L2cap event structure.
Definition: ble_l2cap.h:192
BLE_GAPM_EVT_MAX
@ BLE_GAPM_EVT_MAX
Definition: ble_event.h:109
BLE_GATTS_EVT_WRITE_REQUEST
@ BLE_GATTS_EVT_WRITE_REQUEST
GATTS Write Request event .
Definition: ble_event.h:141
ble_evt_t::sec_evt
ble_sec_evt_t sec_evt
BLE Security Event.
Definition: ble_event.h:203
BLE_GAPC_EVT_CONN_PARAM_UPDATED
@ BLE_GAPC_EVT_CONN_PARAM_UPDATED
Connect Parameter Updated event.
Definition: ble_event.h:120
BLE_SEC_EVT_LINK_ENCRYPTED
@ BLE_SEC_EVT_LINK_ENCRYPTED
Link Encrypted event.
Definition: ble_event.h:167
BLE_GATTS_EVT_NTF_IND
@ BLE_GATTS_EVT_NTF_IND
GATTS Notify or Indicate Complete event .
Definition: ble_event.h:143
BLE_GAPC_EVT_CONNECTED
@ BLE_GAPC_EVT_CONNECTED
Connected event.
Definition: ble_event.h:116
BLE_L2CAP_EVT_ADD_CREDITS_CPLT
@ BLE_L2CAP_EVT_ADD_CREDITS_CPLT
L2cap Credits Add Completed event.
Definition: ble_event.h:183
ble_l2cap.h
BLE L2CAP API.
BLE_L2CAP_EVTS
BLE_L2CAP_EVTS
BLE L2CAP Events.
Definition: ble_event.h:176
BLE_GAPM_EVT_SYNC_STOP
@ BLE_GAPM_EVT_SYNC_STOP
Periodic Advertising Synchronization Stop event.
Definition: ble_event.h:105
BLE_GAPM_EVT_PER_ADV_LIST_SET
@ BLE_GAPM_EVT_PER_ADV_LIST_SET
Periodic Advertising List Set complete event.
Definition: ble_event.h:92
BLE_GATT_COMMON_EVT_BASE
#define BLE_GATT_COMMON_EVT_BASE
BLE GATT Event base.
Definition: ble_event.h:68
BLE_GAPC_EVT_BASE
#define BLE_GAPC_EVT_BASE
BLE GAP Connection Control Event base.
Definition: ble_event.h:65
BLE_GAPC_EVT_PEER_INFO_GOT
@ BLE_GAPC_EVT_PEER_INFO_GOT
Peer Info Get event.
Definition: ble_event.h:124
BLE_GATTS_EVT_MAX
@ BLE_GATTS_EVT_MAX
Definition: ble_event.h:146
ble_gapm_evt_t
BLE GAPM event structure.
Definition: ble_gapm.h:854
ble_sec.h
BLE SEC API.
BLE_GATTC_EVTS
BLE_GATTC_EVTS
BLE GATTC Events.
Definition: ble_event.h:151
BLE_GAPM_EVT_LEPSM_UNREGISTER
@ BLE_GAPM_EVT_LEPSM_UNREGISTER
LEPSM Unregister complete event.
Definition: ble_event.h:95
BLE_COMMON_EVT_MAX
@ BLE_COMMON_EVT_MAX
Definition: ble_event.h:84
BLE_SEC_EVT_KEY_MISSING
@ BLE_SEC_EVT_KEY_MISSING
Key Missing event.
Definition: ble_event.h:170
ble_gapc.h
BLE GAPC API.
BLE_L2CAP_EVT_SDU_RECV
@ BLE_L2CAP_EVT_SDU_RECV
L2cap SDU Receive event.
Definition: ble_event.h:181
BLE_GATT_COMMON_EVT_PRF_REGISTER
@ BLE_GATT_COMMON_EVT_PRF_REGISTER
Service Register event.
Definition: ble_event.h:133
BLE_L2CAP_EVT_MAX
@ BLE_L2CAP_EVT_MAX
Definition: ble_event.h:184
BLE_GATTS_EVT_CCCD_RECOVERY
@ BLE_GATTS_EVT_CCCD_RECOVERY
GATTS CCCD Recovery event .
Definition: ble_event.h:144
BLE_COMMON_EVTS
BLE_COMMON_EVTS
BLE Common Events.
Definition: ble_event.h:82
BLE_GAPM_EVT_WHITELIST_SET
@ BLE_GAPM_EVT_WHITELIST_SET
Whitelist Set complete event.
Definition: ble_event.h:91
BLE_GATTS_EVT_BASE
#define BLE_GATTS_EVT_BASE
BLE GATTS Event base.
Definition: ble_event.h:66
BLE_GAPM_EVT_DEV_INFO_GOT
@ BLE_GAPM_EVT_DEV_INFO_GOT
Device Info Get event.
Definition: ble_event.h:96
BLE_COMMON_EVT_STACK_INIT
@ BLE_COMMON_EVT_STACK_INIT
BLE Stack init complete event.
Definition: ble_event.h:83
BLE_GAPM_EVT_SYNC_ESTABLISH
@ BLE_GAPM_EVT_SYNC_ESTABLISH
Periodic Advertising Synchronization Establish event.
Definition: ble_event.h:104
BLE_GAPC_EVTS
BLE_GAPC_EVTS
BLE GAP Connection Control Events.
Definition: ble_event.h:114
BLE_GATTC_EVT_CHAR_DESC_DISC
@ BLE_GATTC_EVT_CHAR_DESC_DISC
GATTC Characteristic Descriptor Discovery event .
Definition: ble_event.h:156
BLE_GATTC_EVT_PRIMARY_SRVC_DISC
@ BLE_GATTC_EVT_PRIMARY_SRVC_DISC
GATTC Primary Service Discovery event .
Definition: ble_event.h:153
BLE_GATTS_EVT_DATABASE_INITED_IND
@ BLE_GATTS_EVT_DATABASE_INITED_IND
Definition: ble_event.h:145
BLE_L2CAP_EVT_ADD_CREDITS_IND
@ BLE_L2CAP_EVT_ADD_CREDITS_IND
L2cap Credits Add Indicate event.
Definition: ble_event.h:179
BLE_SEC_EVTS
BLE_SEC_EVTS
BLE SEC Events.
Definition: ble_event.h:165
BLE_COMMON_EVT_BASE
#define BLE_COMMON_EVT_BASE
BLE Common Event base.
Definition: ble_event.h:63
ble_evt_t::gapc_evt
ble_gapc_evt_t gapc_evt
BLE GAP Connection Control Event.
Definition: ble_event.h:199
BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ
@ BLE_GAPC_EVT_CONN_PARAM_UPDATE_REQ
Connect Parameter Request event.
Definition: ble_event.h:121
BLE_GAPM_EVT_ADV_DATA_UPDATE
@ BLE_GAPM_EVT_ADV_DATA_UPDATE
Advertising Data update event.
Definition: ble_event.h:100
BLE_L2CAP_EVT_SDU_SEND
@ BLE_L2CAP_EVT_SDU_SEND
L2cap SDU Send event.
Definition: ble_event.h:182
BLE_GATTS_EVTS
BLE_GATTS_EVTS
BLE GATTS Events.
Definition: ble_event.h:139
BLE_GAPM_EVT_SCAN_START
@ BLE_GAPM_EVT_SCAN_START
Scan Start complete event.
Definition: ble_event.h:101
ble_gapc_evt_t
BLE GAPC event structure.
Definition: ble_gapc.h:457
BLE_GATTC_EVT_BASE
#define BLE_GATTC_EVT_BASE
BLE GATTC Event base.
Definition: ble_event.h:67
BLE_GATTC_EVT_CHAR_DISC
@ BLE_GATTC_EVT_CHAR_DISC
GATTC Characteristic Discovery event .
Definition: ble_event.h:155
ble_gatts_evt_t
BLE GATTS event structure.
Definition: ble_gatts.h:405
ble_gapm.h
BLE GAPM API.
BLE_SEC_EVT_KEY_PRESS_NTF
@ BLE_SEC_EVT_KEY_PRESS_NTF
Key Press event.
Definition: ble_event.h:169
BLE_GATTC_EVT_INCLUDE_SRVC_DISC
@ BLE_GATTC_EVT_INCLUDE_SRVC_DISC
GATTC Include Service Discovery event .
Definition: ble_event.h:154
BLE_SEC_EVT_LTK_REQ
@ BLE_SEC_EVT_LTK_REQ
LTK Request event.
Definition: ble_event.h:168
BLE_GATTC_EVT_SRVC_BROWSE
@ BLE_GATTC_EVT_SRVC_BROWSE
GATTC Service Browse event .
Definition: ble_event.h:152
ble_gatt_common_evt_t
GATT Common structure.
Definition: ble_gatt.h:104
BLE_L2CAP_EVT_CONN_IND
@ BLE_L2CAP_EVT_CONN_IND
L2cap Connected Indicate event.
Definition: ble_event.h:178
BLE_SEC_EVT_LINK_ENC_REQUEST
@ BLE_SEC_EVT_LINK_ENC_REQUEST
Link Encrypte Request event.
Definition: ble_event.h:166
BLE_GAPC_EVT_PHY_UPDATED
@ BLE_GAPC_EVT_PHY_UPDATED
PHY Update event.
Definition: ble_event.h:115
ble_evt_handler_t
void(* ble_evt_handler_t)(const ble_evt_t *p_evt)
The BLE event handler type.
Definition: ble_event.h:213
BLE_GAPC_EVT_CONNECT_CANCLE
@ BLE_GAPC_EVT_CONNECT_CANCLE
Connect Cancle event.
Definition: ble_event.h:118
BLE_GAPC_EVT_MAX
@ BLE_GAPC_EVT_MAX
Definition: ble_event.h:126
ble_evt_t
BLE Event Information.
Definition: ble_event.h:193
ble_gattc.h
BLE GATTC API.
BLE_GAPC_EVT_AUTO_CONN_TIMEOUT
@ BLE_GAPC_EVT_AUTO_CONN_TIMEOUT
Auto Connect Timeout event.
Definition: ble_event.h:119
BLE_GAPM_EVT_SCAN_STOP
@ BLE_GAPM_EVT_SCAN_STOP
Scan Stop complete event.
Definition: ble_event.h:102
ble_evt_t::gattc_evt
ble_gattc_evt_t gattc_evt
BLE GATT Client Event.
Definition: ble_event.h:201
BLE_GATTS_EVT_READ_REQUEST
@ BLE_GATTS_EVT_READ_REQUEST
GATTS Read Request event .
Definition: ble_event.h:140
ble_evt_t::gapm_evt
ble_gapm_evt_t gapm_evt
BLE GAP Management Event.
Definition: ble_event.h:198
BLE_GAPM_EVT_READ_RSLV_ADDR
@ BLE_GAPM_EVT_READ_RSLV_ADDR
Read Resolvable Address event.
Definition: ble_event.h:107
BLE_GAPM_EVT_CH_MAP_SET
@ BLE_GAPM_EVT_CH_MAP_SET
Channel Map Set complete event.
Definition: ble_event.h:90
ble_sec_evt_t
BLE Security event structure.
Definition: ble_sec.h:228
BLE_GAPC_EVT_PEER_NAME_GOT
@ BLE_GAPC_EVT_PEER_NAME_GOT
peer Name Get event.
Definition: ble_event.h:122
BLE_L2CAP_EVT_DISCONNECTED
@ BLE_L2CAP_EVT_DISCONNECTED
L2cap Disconnected event.
Definition: ble_event.h:180
BLE_GAPC_EVT_DATA_LENGTH_UPDATED
@ BLE_GAPC_EVT_DATA_LENGTH_UPDATED
Data Length Updated event.
Definition: ble_event.h:125
BLE_GAPM_EVT_LEPSM_REGISTER
@ BLE_GAPM_EVT_LEPSM_REGISTER
LEPSM Register complete event.
Definition: ble_event.h:94
BLE_GAPM_EVT_SYNC_LOST
@ BLE_GAPM_EVT_SYNC_LOST
Periodic Advertising Synchronization Lost event.
Definition: ble_event.h:106
ble_evt_t::gatt_common_evt
ble_gatt_common_evt_t gatt_common_evt
BLE GATT Common Event.
Definition: ble_event.h:202
ble_evt_t::evt_id
uint16_t evt_id
Event ID.
Definition: ble_event.h:194
ble_gattc_evt_t
BLE GATTC event structure.
Definition: ble_gattc.h:289