Macros
Defines
BLE Services » Device Synchronize Service (DSS)
Collaboration diagram for Defines:

## Macros
#define | DSS_SERVICE_UUID
| DSS service UUID. More...
#define | DSS_CONNECTION_MAX 10
| Maximum number of DSS connections. More...
#define | DSS_ROLE_VALUE_LEN 1
| Length of Role characteristic value. More...
#define | DSS_EVT_CNT_VALUE_LEN 4
| Length of Event Count characteristic value. More...
#define | DSS_EVT_PERIOD_VALUE_LEN 2
| Length of Event Period characteristic value. More...
#define | DSS_STATUS_VALUE_LEN 1
| Length of Status characteristic value. More...
#define | DSS_CTRL_PT_VALUE_LEN 7
| Length of Control Point characteristic value. More...
#define | DSS_CTRL_PT_RSP_VAL_LEN 3
| Length of Control Point Response characteristic value. More...
#define | DSS_SYNC_DEV_MAX_NUM 5
| Maximun num of Source Sync Device. More...
#define | DSS_CFG_ADV_IDX 0
| DSS Config Advertising Index. More...
#define | DSS_SYNC_ADV_IDX 1
| DSS Sync Advertising Index. More...

## Detailed Description

## Macro Definition Documentation

## ◆ DSS_CFG_ADV_IDX

#define DSS_CFG_ADV_IDX 0

DSS Config Advertising Index.

Definition at line 82 of file dss.h.

## ◆ DSS_CONNECTION_MAX

#define DSS_CONNECTION_MAX 10

Maximum number of DSS connections.

Definition at line 73 of file dss.h.

## ◆ DSS_CTRL_PT_RSP_VAL_LEN

#define DSS_CTRL_PT_RSP_VAL_LEN 3

Length of Control Point Response characteristic value.

Definition at line 79 of file dss.h.

## ◆ DSS_CTRL_PT_VALUE_LEN

#define DSS_CTRL_PT_VALUE_LEN 7

Length of Control Point characteristic value.

Definition at line 78 of file dss.h.

## ◆ DSS_EVT_CNT_VALUE_LEN

#define DSS_EVT_CNT_VALUE_LEN 4

Length of Event Count characteristic value.

Definition at line 75 of file dss.h.

## ◆ DSS_EVT_PERIOD_VALUE_LEN

#define DSS_EVT_PERIOD_VALUE_LEN 2

Length of Event Period characteristic value.

Definition at line 76 of file dss.h.

## ◆ DSS_ROLE_VALUE_LEN

#define DSS_ROLE_VALUE_LEN 1

Length of Role characteristic value.

Definition at line 74 of file dss.h.

## ◆ DSS_SERVICE_UUID

#define DSS_SERVICE_UUID

Value:
0x1B, 0xD7, 0x90, 0xEC, 0xE8, 0xB9, 0x75, 0x80, \
0x0A, 0x46, 0x44, 0xD3, 0x01, 0x0A, 0xED, 0xA6

DSS service UUID.

Definition at line 71 of file dss.h.

## ◆ DSS_STATUS_VALUE_LEN

#define DSS_STATUS_VALUE_LEN 1

Length of Status characteristic value.

Definition at line 77 of file dss.h.

## ◆ DSS_SYNC_ADV_IDX

#define DSS_SYNC_ADV_IDX 1

DSS Sync Advertising Index.

Definition at line 83 of file dss.h.

## ◆ DSS_SYNC_DEV_MAX_NUM

#define DSS_SYNC_DEV_MAX_NUM 5

Maximun num of Source Sync Device.

Definition at line 81 of file dss.h.