Macros
DMA request definitions
Peripheral Driver » HAL Driver » DMA » Defines » DMA Exported Constants
Collaboration diagram for DMA request definitions:

## Macros
#define | DMA_REQUEST_SPIM_TX LL_DMA_PERIPH_SPIM_TX
| DMA SPIM transmit request More...
#define | DMA_REQUEST_SPIM_RX LL_DMA_PERIPH_SPIM_RX
| DMA SPIM receive request More...
#define | DMA_REQUEST_SPIS_TX LL_DMA_PERIPH_SPIS_TX
| DMA SPIS transmit request More...
#define | DMA_REQUEST_SPIS_RX LL_DMA_PERIPH_SPIS_RX
| DMA SPIS receive request More...
#define | DMA_REQUEST_QSPI0_TX LL_DMA_PERIPH_QSPI0_TX
| DMA QSPI0 transmit request. More...
#define | DMA_REQUEST_QSPI0_RX LL_DMA_PERIPH_QSPI0_RX
| DMA QSPI0 receive request More...
#define | DMA_REQUEST_I2C0_TX LL_DMA_PERIPH_I2C0_TX
| DMA I2C0 transmit request More...
#define | DMA_REQUEST_I2C0_RX LL_DMA_PERIPH_I2C0_RX
| DMA I2C0 receive request More...
#define | DMA_REQUEST_I2C1_TX LL_DMA_PERIPH_I2C1_TX
| DMA I2C1 transmit request More...
#define | DMA_REQUEST_I2C1_RX LL_DMA_PERIPH_I2C1_RX
| DMA I2C1 receive request More...
#define | DMA_REQUEST_I2S_S_TX LL_DMA_PERIPH_I2S_S_TX
| DMA I2S_S transmit request. More...
#define | DMA_REQUEST_I2S_S_RX LL_DMA_PERIPH_I2S_S_RX
| DMA I2S_S receive request More...
#define | DMA_REQUEST_UART0_TX LL_DMA_PERIPH_UART0_TX
| DMA UART0 transmit request. More...
#define | DMA_REQUEST_UART0_RX LL_DMA_PERIPH_UART0_RX
| DMA UART0 receive request More...
#define | DMA_REQUEST_QSPI1_TX LL_DMA_PERIPH_QSPI1_TX
| DMA QSPI1 transmit request. More...
#define | DMA_REQUEST_QSPI1_RX LL_DMA_PERIPH_QSPI1_RX
| DMA QSPI1 receive request More...
#define | DMA_REQUEST_I2S_M_TX LL_DMA_PERIPH_I2S_M_TX
| DMA I2S_M transmit request. More...
#define | DMA_REQUEST_I2S_M_RX LL_DMA_PERIPH_I2S_M_RX
| DMA I2S_M receive request More...
#define | DMA_REQUEST_SNSADC LL_DMA_PERIPH_SNSADC
| DMA SenseADC request More...
#define | DMA_REQUEST_MEM LL_DMA_PERIPH_MEM
| DMA Memory request More...
#define | DMA0_REQUEST_SPIM_TX DMA_REQUEST_SPIM_TX
| DMA SPIM transmit request More...
#define | DMA0_REQUEST_SPIM_RX DMA_REQUEST_SPIM_RX
| DMA SPIM receive request More...
#define | DMA0_REQUEST_SPIS_TX DMA_REQUEST_SPIS_TX
| DMA SPIS transmit request More...
#define | DMA0_REQUEST_SPIS_RX DMA_REQUEST_SPIS_RX
| DMA SPIS receive request More...
#define | DMA0_REQUEST_QSPI0_TX DMA_REQUEST_QSPI0_TX
| DMA QSPI0 transmit request. More...
#define | DMA0_REQUEST_QSPI0_RX DMA_REQUEST_QSPI0_RX
| DMA QSPI0 receive request More...
#define | DMA0_REQUEST_I2C0_TX DMA_REQUEST_I2C0_TX
| DMA I2C0 transmit request More...
#define | DMA0_REQUEST_I2C0_RX DMA_REQUEST_I2C0_RX
| DMA I2C0 receive request More...
#define | DMA0_REQUEST_I2C1_TX DMA_REQUEST_I2C1_TX
| DMA I2C1 transmit request More...
#define | DMA0_REQUEST_I2C1_RX DMA_REQUEST_I2C1_RX
| DMA I2C1 receive request More...
#define | DMA0_REQUEST_I2S_S_TX DMA_REQUEST_I2S_S_TX
| DMA I2S_S transmit request. More...
#define | DMA0_REQUEST_I2S_S_RX DMA_REQUEST_I2S_S_RX
| DMA I2S_S receive request More...
#define | DMA0_REQUEST_UART0_TX DMA_REQUEST_UART0_TX
| DMA UART0 transmit request. More...
#define | DMA0_REQUEST_UART0_RX DMA_REQUEST_UART0_RX
| DMA UART0 receive request More...
#define | DMA0_REQUEST_QSPI1_TX DMA_REQUEST_QSPI1_TX
| DMA QSPI1 transmit request. More...
#define | DMA0_REQUEST_QSPI1_RX DMA_REQUEST_QSPI1_RX
| DMA QSPI1 receive request More...
#define | DMA0_REQUEST_I2S_M_TX DMA_REQUEST_I2S_M_TX
| DMA I2S_M transmit request. More...
#define | DMA0_REQUEST_I2S_M_RX DMA_REQUEST_I2S_M_RX
| DMA I2S_M receive request More...
#define | DMA0_REQUEST_SNSADC DMA_REQUEST_SNSADC
| DMA SenseADC request More...
#define | DMA0_REQUEST_MEM DMA_REQUEST_MEM
| DMA Memory request More...

## Detailed Description

## Macro Definition Documentation

## ◆ DMA0_REQUEST_I2C0_RX

#define DMA0_REQUEST_I2C0_RX DMA_REQUEST_I2C0_RX

DMA I2C0 receive request

Definition at line 258 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C0_TX

#define DMA0_REQUEST_I2C0_TX DMA_REQUEST_I2C0_TX

DMA I2C0 transmit request

Definition at line 257 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C1_RX

#define DMA0_REQUEST_I2C1_RX DMA_REQUEST_I2C1_RX

DMA I2C1 receive request

Definition at line 260 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2C1_TX

#define DMA0_REQUEST_I2C1_TX DMA_REQUEST_I2C1_TX

DMA I2C1 transmit request

Definition at line 259 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2S_M_RX

#define DMA0_REQUEST_I2S_M_RX DMA_REQUEST_I2S_M_RX

DMA I2S_M receive request

Definition at line 268 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2S_M_TX

#define DMA0_REQUEST_I2S_M_TX DMA_REQUEST_I2S_M_TX

DMA I2S_M transmit request.

Definition at line 267 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2S_S_RX

#define DMA0_REQUEST_I2S_S_RX DMA_REQUEST_I2S_S_RX

DMA I2S_S receive request

Definition at line 262 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_I2S_S_TX

#define DMA0_REQUEST_I2S_S_TX DMA_REQUEST_I2S_S_TX

DMA I2S_S transmit request.

Definition at line 261 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_MEM

#define DMA0_REQUEST_MEM DMA_REQUEST_MEM

DMA Memory request

Definition at line 270 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI0_RX

#define DMA0_REQUEST_QSPI0_RX DMA_REQUEST_QSPI0_RX

DMA QSPI0 receive request

Definition at line 256 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI0_TX

#define DMA0_REQUEST_QSPI0_TX DMA_REQUEST_QSPI0_TX

DMA QSPI0 transmit request.

Definition at line 255 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI1_RX

#define DMA0_REQUEST_QSPI1_RX DMA_REQUEST_QSPI1_RX

DMA QSPI1 receive request

Definition at line 266 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_QSPI1_TX

#define DMA0_REQUEST_QSPI1_TX DMA_REQUEST_QSPI1_TX

DMA QSPI1 transmit request.

Definition at line 265 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SNSADC

#define DMA0_REQUEST_SNSADC DMA_REQUEST_SNSADC

DMA SenseADC request

Definition at line 269 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIM_RX

#define DMA0_REQUEST_SPIM_RX DMA_REQUEST_SPIM_RX

DMA SPIM receive request

Definition at line 252 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIM_TX

#define DMA0_REQUEST_SPIM_TX DMA_REQUEST_SPIM_TX

DMA SPIM transmit request

Definition at line 251 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIS_RX

#define DMA0_REQUEST_SPIS_RX DMA_REQUEST_SPIS_RX

DMA SPIS receive request

Definition at line 254 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_SPIS_TX

#define DMA0_REQUEST_SPIS_TX DMA_REQUEST_SPIS_TX

DMA SPIS transmit request

Definition at line 253 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART0_RX

#define DMA0_REQUEST_UART0_RX DMA_REQUEST_UART0_RX

DMA UART0 receive request

Definition at line 264 of file gr55xx_hal_dma.h.

## ◆ DMA0_REQUEST_UART0_TX

#define DMA0_REQUEST_UART0_TX DMA_REQUEST_UART0_TX

DMA UART0 transmit request.

Definition at line 263 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2C0_RX

#define DMA_REQUEST_I2C0_RX LL_DMA_PERIPH_I2C0_RX

DMA I2C0 receive request

Definition at line 237 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2C0_TX

#define DMA_REQUEST_I2C0_TX LL_DMA_PERIPH_I2C0_TX

DMA I2C0 transmit request

Definition at line 236 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2C1_RX

#define DMA_REQUEST_I2C1_RX LL_DMA_PERIPH_I2C1_RX

DMA I2C1 receive request

Definition at line 239 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2C1_TX

#define DMA_REQUEST_I2C1_TX LL_DMA_PERIPH_I2C1_TX

DMA I2C1 transmit request

Definition at line 238 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2S_M_RX

#define DMA_REQUEST_I2S_M_RX LL_DMA_PERIPH_I2S_M_RX

DMA I2S_M receive request

Definition at line 247 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2S_M_TX

#define DMA_REQUEST_I2S_M_TX LL_DMA_PERIPH_I2S_M_TX

DMA I2S_M transmit request.

Definition at line 246 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2S_S_RX

#define DMA_REQUEST_I2S_S_RX LL_DMA_PERIPH_I2S_S_RX

DMA I2S_S receive request

Definition at line 241 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_I2S_S_TX

#define DMA_REQUEST_I2S_S_TX LL_DMA_PERIPH_I2S_S_TX

DMA I2S_S transmit request.

Definition at line 240 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_MEM

#define DMA_REQUEST_MEM LL_DMA_PERIPH_MEM

DMA Memory request

Definition at line 249 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_QSPI0_RX

#define DMA_REQUEST_QSPI0_RX LL_DMA_PERIPH_QSPI0_RX

DMA QSPI0 receive request

Definition at line 235 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_QSPI0_TX

#define DMA_REQUEST_QSPI0_TX LL_DMA_PERIPH_QSPI0_TX

DMA QSPI0 transmit request.

Definition at line 234 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_QSPI1_RX

#define DMA_REQUEST_QSPI1_RX LL_DMA_PERIPH_QSPI1_RX

DMA QSPI1 receive request

Definition at line 245 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_QSPI1_TX

#define DMA_REQUEST_QSPI1_TX LL_DMA_PERIPH_QSPI1_TX

DMA QSPI1 transmit request.

Definition at line 244 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_SNSADC

#define DMA_REQUEST_SNSADC LL_DMA_PERIPH_SNSADC

DMA SenseADC request

Definition at line 248 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_SPIM_RX

#define DMA_REQUEST_SPIM_RX LL_DMA_PERIPH_SPIM_RX

DMA SPIM receive request

Definition at line 231 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_SPIM_TX

#define DMA_REQUEST_SPIM_TX LL_DMA_PERIPH_SPIM_TX

DMA SPIM transmit request

Definition at line 230 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_SPIS_RX

#define DMA_REQUEST_SPIS_RX LL_DMA_PERIPH_SPIS_RX

DMA SPIS receive request

Definition at line 233 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_SPIS_TX

#define DMA_REQUEST_SPIS_TX LL_DMA_PERIPH_SPIS_TX

DMA SPIS transmit request

Definition at line 232 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_UART0_RX

#define DMA_REQUEST_UART0_RX LL_DMA_PERIPH_UART0_RX

DMA UART0 receive request

Definition at line 243 of file gr55xx_hal_dma.h.

## ◆ DMA_REQUEST_UART0_TX

#define DMA_REQUEST_UART0_TX LL_DMA_PERIPH_UART0_TX

DMA UART0 transmit request.

Definition at line 242 of file gr55xx_hal_dma.h.