Macros
Current Time Adjust Reason
BLE Services » Current Time Service (CTS) » Defines

Current Time Service Adjust Reason. More...

Collaboration diagram for Current Time Adjust Reason:

## Macros
#define | CTS_AR_NO_CHANGE (0x00 << 0)
| No change for current time. More...
#define | CTS_AR_MAUAL_TIME_UPDATE (0x01 << 0)
| Manual time update. More...
#define | CTS_AR_EXT_REF_TIME_UPDATE (0x01 << 1)
| External reference time update. More...
#define | CTS_AR_TIME_ZONE_CHANGE (0x01 << 2)
| Change of time zone. More...
#define | CTS_AR_DST_CHANGE (0x01 << 3)
| Change of DST (daylight savings time). More...

## Detailed Description

Current Time Service Adjust Reason.

## Macro Definition Documentation

## ◆ CTS_AR_DST_CHANGE

#define CTS_AR_DST_CHANGE (0x01 << 3)

Change of DST (daylight savings time).

Definition at line 104 of file cts.h.

## ◆ CTS_AR_EXT_REF_TIME_UPDATE

#define CTS_AR_EXT_REF_TIME_UPDATE (0x01 << 1)

External reference time update.

Definition at line 102 of file cts.h.

## ◆ CTS_AR_MAUAL_TIME_UPDATE

#define CTS_AR_MAUAL_TIME_UPDATE (0x01 << 0)

Manual time update.

Definition at line 101 of file cts.h.

## ◆ CTS_AR_NO_CHANGE

#define CTS_AR_NO_CHANGE (0x00 << 0)

No change for current time.

Definition at line 100 of file cts.h.

## ◆ CTS_AR_TIME_ZONE_CHANGE

#define CTS_AR_TIME_ZONE_CHANGE (0x01 << 2)

Change of time zone.

Definition at line 103 of file cts.h.