Macros
Hash Mode
Peripheral Driver » LL Driver » HMAC » Defines » HMAC Exported Constants
Collaboration diagram for Hash Mode:

## Macros
#define | LL_HMAC_HASH_STANDARD 0x00000000U
| Standard Mode. More...
#define | LL_HMAC_HASH_USER (1UL << HMAC_CONFIG_ENABLE_USERHASH)
| User Mode More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_HMAC_HASH_STANDARD

#define LL_HMAC_HASH_STANDARD 0x00000000U

Standard Mode.

Definition at line 112 of file gr55xx_ll_hmac.h.

## ◆ LL_HMAC_HASH_USER

#define LL_HMAC_HASH_USER (1UL << HMAC_CONFIG_ENABLE_USERHASH)

User Mode

Definition at line 113 of file gr55xx_ll_hmac.h.