Enumerations
Enumerations
BLE Services » Device Information Service Client (DIS_C)
Collaboration diagram for Enumerations:

## Enumerations
enum | dis_c_evt_type_t { DIS_C_EVT_INVALID, DIS_C_EVT_DISCOVERY_COMPLETE, DIS_C_EVT_DISCOVERY_FAIL, DIS_C_EVT_DEV_INFORMATION_READ_RSP }
| Device Information Service Client event type. More...
enum | dis_c_char_type_t { DIS_C_SYS_ID, DIS_C_MODEL_NUM, DIS_C_SERIAL_NUM, DIS_C_HW_REV, DIS_C_FW_REV, DIS_C_SW_REV, DIS_C_MANUF_NAME, DIS_C_CERT_LIST, DIS_C_PNP_ID, DIS_C_CHARACTER_NB }
| Device Information Service Client characteristic type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ dis_c_char_type_t

enum dis_c_char_type_t

Device Information Service Client characteristic type.

Enumerator
DIS_C_SYS_ID | System ID characteristic.
DIS_C_MODEL_NUM | Model Number String characteristic.
DIS_C_SERIAL_NUM | Serial Number String characteristic.
DIS_C_HW_REV | Hardware Revision String characteristic.
DIS_C_FW_REV | Firmware Revision String characteristic.
DIS_C_SW_REV | Software Revision String characteristic.
DIS_C_MANUF_NAME | Manufacturer Name String characteristic.
DIS_C_CERT_LIST | IEEE 11073-20601 Regulatory Certification Data List characteristic.
DIS_C_PNP_ID | PnP ID characteristic.
DIS_C_CHARACTER_NB | Number of all Device Information Service characteristics.

Definition at line 98 of file dis_c.h.

## ◆ dis_c_evt_type_t

enum dis_c_evt_type_t

Device Information Service Client event type.

Enumerator
DIS_C_EVT_INVALID | DIS Client invalid event.
DIS_C_EVT_DISCOVERY_COMPLETE | DIS Client has found Device Information Service and its characteristics.
DIS_C_EVT_DISCOVERY_FAIL | DIS Client found DIS service failed because of invalid operation or no found at the peer.
DIS_C_EVT_DEV_INFORMATION_READ_RSP | DIS Client has received device information value read response.

Definition at line 89 of file dis_c.h.