Enumerations
Enumerations
BLE Services » Tx Power Service Client (TPS_C)
Collaboration diagram for Enumerations:

## Enumerations
enum | tps_c_evt_type_t { TPS_C_EVT_INVALID, TPS_C_EVT_DISCOVERY_COMPLETE, TPS_C_EVT_DISCOVERY_FAIL, TPS_C_EVT_TX_POWER_LEVEL_RECEIVE }
| Tx Power Service Client event type. More...

## Detailed Description

## Enumeration Type Documentation

## ◆ tps_c_evt_type_t

enum tps_c_evt_type_t

Tx Power Service Client event type.

Enumerator
TPS_C_EVT_INVALID | TPS Client invalid event.
TPS_C_EVT_DISCOVERY_COMPLETE | TPS Client has found TPS service and its characteristics.
TPS_C_EVT_DISCOVERY_FAIL | TPS Client found TPS service failed because of invalid operation or no found at the peer.
TPS_C_EVT_TX_POWER_LEVEL_RECEIVE | TPS Client has received Tx Power Level value.

Definition at line 77 of file tps_c.h.