Functions
Functions
BLE Services » Blood Pressure Service (BPS)
Collaboration diagram for Functions:

## Functions
sdk_err_t | bps_service_init (bps_init_t *p_bps_init)
| Initialize a Blood Pressure Service instance and add in the DB. More...
sdk_err_t | bps_measurement_send (uint8_t conn_idx, bps_meas_t *p_meas)
| Send Blood Pressure Measurement indication. More...

## Detailed Description

## Function Documentation

## ◆ bps_measurement_send()

sdk_err_t bps_measurement_send | ( | uint8_t | conn_idx,
|  | bps_meas_t * | p_meas
| ) |  |

Send Blood Pressure Measurement indication.

Parameters

  [in] | conn_idx | Connection index.
  [in] | p_meas | Pointer to the Blood Pressure measurement.

Returns
  Result of sending indication.

## ◆ bps_service_init()

sdk_err_t bps_service_init | ( | bps_init_t * | p_bps_init | ) |

Initialize a Blood Pressure Service instance and add in the DB.

Parameters

  [in] | p_bps_init | Pointer to Blood Pressure Service initialization variable

Returns
  Result of service initialization.