Public Attributes | List of all members
app_iso7816_pin_t Struct Reference
Peripheral Driver » APP DRIVER » ISO7816 » Structures

ISO7816 IO configuration Structures. More...

`#include <app_iso7816.h>`

## Public Attributes
app_io_type_t | type
| Specifies the type of IO. More...
app_io_mux_t | mux
| Specifies the Peripheral to be connected to the selected pins. More...
uint32_t | pin
| Specifies the IO pins to be configured. More...
app_io_pull_t | pull
| Specifies the Pull-up or Pull-Down activation for the selected pins. More...

## Detailed Description

ISO7816 IO configuration Structures.

Definition at line 170 of file app_iso7816.h.

## Member Data Documentation

## ◆ mux

app_io_mux_t app_iso7816_pin_t::mux

Specifies the Peripheral to be connected to the selected pins.

Definition at line 173 of file app_iso7816.h.

## ◆ pin

uint32_t app_iso7816_pin_t::pin

Specifies the IO pins to be configured.

This parameter can be any value of Defines.

Definition at line 174 of file app_iso7816.h.

## ◆ pull

app_io_pull_t app_iso7816_pin_t::pull

Specifies the Pull-up or Pull-Down activation for the selected pins.

Definition at line 176 of file app_iso7816.h.

## ◆ type

app_io_type_t app_iso7816_pin_t::type

Specifies the type of IO.

Definition at line 172 of file app_iso7816.h.

The documentation for this struct was generated from the following file:

- app_iso7816.h