Macros
Source data alignment
Peripheral Driver » LL Driver » DMA » Defines » DMA Exported Constants
Collaboration diagram for Source data alignment:

## Macros
#define | LL_DMA_SDATAALIGN_BYTE DMA_CTLL_SRC_TR_WIDTH_8
| Source data alignment : Byte More...
#define | LL_DMA_SDATAALIGN_HALFWORD DMA_CTLL_SRC_TR_WIDTH_16
| Source data alignment : HalfWord. More...
#define | LL_DMA_SDATAALIGN_WORD DMA_CTLL_SRC_TR_WIDTH_32
| Source data alignment : Word More...

## Detailed Description

## Macro Definition Documentation

## ◆ LL_DMA_SDATAALIGN_BYTE

#define LL_DMA_SDATAALIGN_BYTE DMA_CTLL_SRC_TR_WIDTH_8

Source data alignment : Byte

Definition at line 230 of file gr55xx_ll_dma.h.

## ◆ LL_DMA_SDATAALIGN_HALFWORD

#define LL_DMA_SDATAALIGN_HALFWORD DMA_CTLL_SRC_TR_WIDTH_16

Source data alignment : HalfWord.

Definition at line 231 of file gr55xx_ll_dma.h.

## ◆ LL_DMA_SDATAALIGN_WORD

#define LL_DMA_SDATAALIGN_WORD DMA_CTLL_SRC_TR_WIDTH_32

Source data alignment : Word

Definition at line 232 of file gr55xx_ll_dma.h.