Macros
Attribute and Service Access Rights
BLE » Generic Attribute Profile (GATT) » Generic Attribute Profile (GATT) Server » Defines

## Macros
#define | BLE_GATTS_NOAUTH (0x00)
#define | BLE_GATTS_UNAUTH (0x01)
#define | BLE_GATTS_AUTH (0x02)
#define | BLE_GATTS_SEC_CON (0x03)

## Detailed Description

## Macro Definition Documentation

## ◆ BLE_GATTS_AUTH

#define BLE_GATTS_AUTH (0x02)

LE security mode 1, level 3. Link needs to be encrypted and authenticated (MITM). Parameter of Service Permission, BLE_GATTS_READ_PERM, BLE_GATTS_WRITE_REQ_PERM, BLE_GATTS_WRITE_CMD_PERM, BLE_GATTS_WRITE_SIGNED_PERM, BLE_GATTS_INDICATE_PERM, BLE_GATTS_NOTIFY_PERM.

Definition at line 102 of file ble_gatts.h.

## ◆ BLE_GATTS_NOAUTH

#define BLE_GATTS_NOAUTH (0x00)

LE security mode 1, level 1. Link does not need to be encrypted or authenticated. Parameter of Service Permission, BLE_GATTS_READ_PERM, BLE_GATTS_WRITE_REQ_PERM, BLE_GATTS_WRITE_CMD_PERM, BLE_GATTS_WRITE_SIGNED_PERM, BLE_GATTS_INDICATE_PERM, BLE_GATTS_NOTIFY_PERM.

Definition at line 98 of file ble_gatts.h.

## ◆ BLE_GATTS_SEC_CON

#define BLE_GATTS_SEC_CON (0x03)

LE security mode 1, level 4. Link needs to be encrypted and authenticateBLE_GATTS_d (secure connections). Parameter of Service Permission, BLE_GATTS_READ_PERM, BLE_GATTS_WRITE_REQ_PERM, BLE_GATTS_WRITE_CMD_PERM, BLE_GATTS_WRITE_SIGNED_PERM, BLE_GATTS_INDICATE_PERM, BLE_GATTS_NOTIFY_PERM.

Definition at line 104 of file ble_gatts.h.

## ◆ BLE_GATTS_UNAUTH

#define BLE_GATTS_UNAUTH (0x01)

LE security mode 1, level 2. Link needs to be encrypted, but not to be authenticated. Parameter of Service Permission, BLE_GATTS_READ_PERM, BLE_GATTS_WRITE_REQ_PERM, BLE_GATTS_WRITE_CMD_PERM, BLE_GATTS_WRITE_SIGNED_PERM, BLE_GATTS_INDICATE_PERM, BLE_GATTS_NOTIFY_PERM.

Definition at line 100 of file ble_gatts.h.