Macros
SPI Data Size
Peripheral Driver » HAL Driver » SPI » Defines » SPI Exported Constants

## Macros
#define | SPI_DATASIZE_4BIT LL_SSI_DATASIZE_4BIT
#define | SPI_DATASIZE_5BIT LL_SSI_DATASIZE_5BIT
#define | SPI_DATASIZE_6BIT LL_SSI_DATASIZE_6BIT
#define | SPI_DATASIZE_7BIT LL_SSI_DATASIZE_7BIT
#define | SPI_DATASIZE_8BIT LL_SSI_DATASIZE_8BIT
#define | SPI_DATASIZE_9BIT LL_SSI_DATASIZE_9BIT
#define | SPI_DATASIZE_10BIT LL_SSI_DATASIZE_10BIT
#define | SPI_DATASIZE_11BIT LL_SSI_DATASIZE_11BIT
#define | SPI_DATASIZE_12BIT LL_SSI_DATASIZE_12BIT
#define | SPI_DATASIZE_13BIT LL_SSI_DATASIZE_13BIT
#define | SPI_DATASIZE_14BIT LL_SSI_DATASIZE_14BIT
#define | SPI_DATASIZE_15BIT LL_SSI_DATASIZE_15BIT
#define | SPI_DATASIZE_16BIT LL_SSI_DATASIZE_16BIT
#define | SPI_DATASIZE_17BIT LL_SSI_DATASIZE_17BIT
#define | SPI_DATASIZE_18BIT LL_SSI_DATASIZE_18BIT
#define | SPI_DATASIZE_19BIT LL_SSI_DATASIZE_19BIT
#define | SPI_DATASIZE_20BIT LL_SSI_DATASIZE_20BIT
#define | SPI_DATASIZE_21BIT LL_SSI_DATASIZE_21BIT
#define | SPI_DATASIZE_22BIT LL_SSI_DATASIZE_22BIT
#define | SPI_DATASIZE_23BIT LL_SSI_DATASIZE_23BIT
#define | SPI_DATASIZE_24BIT LL_SSI_DATASIZE_24BIT
#define | SPI_DATASIZE_25BIT LL_SSI_DATASIZE_25BIT
#define | SPI_DATASIZE_26BIT LL_SSI_DATASIZE_26BIT
#define | SPI_DATASIZE_27BIT LL_SSI_DATASIZE_27BIT
#define | SPI_DATASIZE_28BIT LL_SSI_DATASIZE_28BIT
#define | SPI_DATASIZE_29BIT LL_SSI_DATASIZE_29BIT
#define | SPI_DATASIZE_30BIT LL_SSI_DATASIZE_30BIT
#define | SPI_DATASIZE_31BIT LL_SSI_DATASIZE_31BIT
#define | SPI_DATASIZE_32BIT LL_SSI_DATASIZE_32BIT

## Detailed Description

## Macro Definition Documentation

## ◆ SPI_DATASIZE_10BIT

#define SPI_DATASIZE_10BIT LL_SSI_DATASIZE_10BIT

10-bit serial data transfer

Definition at line 245 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_11BIT

#define SPI_DATASIZE_11BIT LL_SSI_DATASIZE_11BIT

11-bit serial data transfer

Definition at line 246 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_12BIT

#define SPI_DATASIZE_12BIT LL_SSI_DATASIZE_12BIT

12-bit serial data transfer

Definition at line 247 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_13BIT

#define SPI_DATASIZE_13BIT LL_SSI_DATASIZE_13BIT

13-bit serial data transfer

Definition at line 248 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_14BIT

#define SPI_DATASIZE_14BIT LL_SSI_DATASIZE_14BIT

14-bit serial data transfer

Definition at line 249 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_15BIT

#define SPI_DATASIZE_15BIT LL_SSI_DATASIZE_15BIT

15-bit serial data transfer

Definition at line 250 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_16BIT

#define SPI_DATASIZE_16BIT LL_SSI_DATASIZE_16BIT

16-bit serial data transfer

Definition at line 251 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_17BIT

#define SPI_DATASIZE_17BIT LL_SSI_DATASIZE_17BIT

17-bit serial data transfer

Definition at line 252 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_18BIT

#define SPI_DATASIZE_18BIT LL_SSI_DATASIZE_18BIT

18-bit serial data transfer

Definition at line 253 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_19BIT

#define SPI_DATASIZE_19BIT LL_SSI_DATASIZE_19BIT

19-bit serial data transfer

Definition at line 254 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_20BIT

#define SPI_DATASIZE_20BIT LL_SSI_DATASIZE_20BIT

20-bit serial data transfer

Definition at line 255 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_21BIT

#define SPI_DATASIZE_21BIT LL_SSI_DATASIZE_21BIT

21-bit serial data transfer

Definition at line 256 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_22BIT

#define SPI_DATASIZE_22BIT LL_SSI_DATASIZE_22BIT

22-bit serial data transfer

Definition at line 257 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_23BIT

#define SPI_DATASIZE_23BIT LL_SSI_DATASIZE_23BIT

23-bit serial data transfer

Definition at line 258 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_24BIT

#define SPI_DATASIZE_24BIT LL_SSI_DATASIZE_24BIT

24-bit serial data transfer

Definition at line 259 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_25BIT

#define SPI_DATASIZE_25BIT LL_SSI_DATASIZE_25BIT

25-bit serial data transfer

Definition at line 260 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_26BIT

#define SPI_DATASIZE_26BIT LL_SSI_DATASIZE_26BIT

26-bit serial data transfer

Definition at line 261 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_27BIT

#define SPI_DATASIZE_27BIT LL_SSI_DATASIZE_27BIT

27-bit serial data transfer

Definition at line 262 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_28BIT

#define SPI_DATASIZE_28BIT LL_SSI_DATASIZE_28BIT

28-bit serial data transfer

Definition at line 263 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_29BIT

#define SPI_DATASIZE_29BIT LL_SSI_DATASIZE_29BIT

29-bit serial data transfer

Definition at line 264 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_30BIT

#define SPI_DATASIZE_30BIT LL_SSI_DATASIZE_30BIT

30-bit serial data transfer

Definition at line 265 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_31BIT

#define SPI_DATASIZE_31BIT LL_SSI_DATASIZE_31BIT

31-bit serial data transfer

Definition at line 266 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_32BIT

#define SPI_DATASIZE_32BIT LL_SSI_DATASIZE_32BIT

32-bit serial data transfer

Definition at line 267 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_4BIT

#define SPI_DATASIZE_4BIT LL_SSI_DATASIZE_4BIT

4-bit serial data transfer

Definition at line 239 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_5BIT

#define SPI_DATASIZE_5BIT LL_SSI_DATASIZE_5BIT

5-bit serial data transfer

Definition at line 240 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_6BIT

#define SPI_DATASIZE_6BIT LL_SSI_DATASIZE_6BIT

6-bit serial data transfer

Definition at line 241 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_7BIT

#define SPI_DATASIZE_7BIT LL_SSI_DATASIZE_7BIT

7-bit serial data transfer

Definition at line 242 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_8BIT

#define SPI_DATASIZE_8BIT LL_SSI_DATASIZE_8BIT

8-bit serial data transfer

Definition at line 243 of file gr55xx_hal_spi.h.

## ◆ SPI_DATASIZE_9BIT

#define SPI_DATASIZE_9BIT LL_SSI_DATASIZE_9BIT

9-bit serial data transfer

Definition at line 244 of file gr55xx_hal_spi.h.