Macros
app_qspi_user_config.h File Reference

Go to the source code of this file.

## Macros
#define | QSPI_SYNC_SCROLL_DRAW_SCREEN_SUPPORT 1u
#define | QSPI_ASYNC_SCROLL_DRAW_SCREEN_SUPPORT 1u
#define | QSPI_ASYNC_VERI_LINK_DRAW_SCREEN_SUPPORT 1u
#define | QSPI_LLP_WRITE_PSRAM_SUPPORT 1u
#define | QSPI_BLIT_RECT_IMAGE_SUPPORT 0u
#define | QSPI_DMA_LLP_FEATUTE_SUPPORT
#define | DMA_LLP_BLOCKS_FOR_WRITE 48u
#define | DMA_LLP_BLOCKS_FOR_BLIT 32u

## Macro Definition Documentation

## ◆ DMA_LLP_BLOCKS_FOR_BLIT

#define DMA_LLP_BLOCKS_FOR_BLIT 32u

Definition at line 102 of file app_qspi_user_config.h.

## ◆ DMA_LLP_BLOCKS_FOR_WRITE

#define DMA_LLP_BLOCKS_FOR_WRITE 48u

Definition at line 94 of file app_qspi_user_config.h.

## ◆ QSPI_ASYNC_SCROLL_DRAW_SCREEN_SUPPORT

#define QSPI_ASYNC_SCROLL_DRAW_SCREEN_SUPPORT 1u

Definition at line 38 of file app_qspi_user_config.h.

## ◆ QSPI_ASYNC_VERI_LINK_DRAW_SCREEN_SUPPORT

#define QSPI_ASYNC_VERI_LINK_DRAW_SCREEN_SUPPORT 1u

Definition at line 52 of file app_qspi_user_config.h.

## ◆ QSPI_BLIT_RECT_IMAGE_SUPPORT

#define QSPI_BLIT_RECT_IMAGE_SUPPORT 0u

Definition at line 72 of file app_qspi_user_config.h.

## ◆ QSPI_DMA_LLP_FEATUTE_SUPPORT

#define QSPI_DMA_LLP_FEATUTE_SUPPORT

Value:
(QSPI_SYNC_SCROLL_DRAW_SCREEN_SUPPORT || \
QSPI_ASYNC_SCROLL_DRAW_SCREEN_SUPPORT || \
QSPI_ASYNC_VERI_LINK_DRAW_SCREEN_SUPPORT || \
QSPI_LLP_WRITE_PSRAM_SUPPORT )

Definition at line 83 of file app_qspi_user_config.h.

## ◆ QSPI_LLP_WRITE_PSRAM_SUPPORT

#define QSPI_LLP_WRITE_PSRAM_SUPPORT 1u

Definition at line 62 of file app_qspi_user_config.h.

## ◆ QSPI_SYNC_SCROLL_DRAW_SCREEN_SUPPORT

#define QSPI_SYNC_SCROLL_DRAW_SCREEN_SUPPORT 1u

Definition at line 23 of file app_qspi_user_config.h.

QSPI_SYNC_SCROLL_DRAW_SCREEN_SUPPORT
#define QSPI_SYNC_SCROLL_DRAW_SCREEN_SUPPORT
Definition: app_qspi_user_config.h:23