Public Attributes | List of all members
_msio_init Struct Reference
Peripheral Driver » HAL Driver » MSIO » Structures

MSIO init structure definition. More...

`#include <gr55xx_hal_msio.h>`

## Public Attributes
uint32_t | pin
uint32_t | direction
uint32_t | mode
uint32_t | pull
uint32_t | mux

## Detailed Description

MSIO init structure definition.

Definition at line 86 of file gr55xx_hal_msio.h.

## Member Data Documentation

## ◆ direction

uint32_t _msio_init::direction

Specifies the direction for the selected pins. This parameter can be a value of MSIO direction

Definition at line 91 of file gr55xx_hal_msio.h.

## ◆ mode

uint32_t _msio_init::mode

Specifies the operating mode for the selected pins. This parameter can be a value of MSIO mode

Definition at line 94 of file gr55xx_hal_msio.h.

## ◆ mux

uint32_t _msio_init::mux

Specifies the Peripheral to be connected to the selected pins. This parameter can be a value of GPIOEx Mux function selection.

Definition at line 100 of file gr55xx_hal_msio.h.

## ◆ pin

uint32_t _msio_init::pin

Specifies the MSIO pins to be configured. This parameter can be any value of MSIO pins

Definition at line 88 of file gr55xx_hal_msio.h.

## ◆ pull

uint32_t _msio_init::pull

Specifies the Pull-up or Pull-Down activation for the selected pins. This parameter can be a value of MSIO pull

Definition at line 97 of file gr55xx_hal_msio.h.

The documentation for this struct was generated from the following file:

- gr55xx_hal_msio.h