Macros
Power States Defines
Peripheral Driver » APP DRIVER » ISO7816 » Defines

## Macros
#define | APP_ISO7816_PWR_STATE_OFF HAL_ISO7816_PWR_STATE_OFF
#define | APP_ISO7816_PWR_STATE_PWRUP_VCC HAL_ISO7816_PWR_STATE_PWRUP_VCC
#define | APP_ISO7816_PWR_STATE_PWRUP_RST HAL_ISO7816_PWR_STATE_PWRUP_RST
#define | APP_ISO7816_PWR_STATE_PWRDN_RST HAL_ISO7816_PWR_STATE_PWRDN_RST
#define | APP_ISO7816_PWR_STATE_PWRDN_VCC HAL_ISO7816_PWR_STATE_PWRDN_VCC
#define | APP_ISO7816_PWR_STATE_STOP_PRE HAL_ISO7816_PWR_STATE_STOP_PRE
#define | APP_ISO7816_PWR_STATE_STOP HAL_ISO7816_PWR_STATE_STOP
#define | APP_ISO7816_PWR_STATE_STOP_POST HAL_ISO7816_PWR_STATE_STOP_POST
#define | APP_ISO7816_PWR_STATE_IDLE HAL_ISO7816_PWR_STATE_IDLE
#define | APP_ISO7816_PWR_STATE_RX_TS0 HAL_ISO7816_PWR_STATE_RX_TS0
#define | APP_ISO7816_PWR_STATE_RX_TS1 HAL_ISO7816_PWR_STATE_RX_TS1
#define | APP_ISO7816_PWR_STATE_RX HAL_ISO7816_PWR_STATE_RX
#define | APP_ISO7816_PWR_STATE_TX HAL_ISO7816_PWR_STATE_TX
#define | APP_ISO7816_PWR_STATE_TX_RX HAL_ISO7816_PWR_STATE_TX_RX

## Detailed Description

## Macro Definition Documentation

## ◆ APP_ISO7816_PWR_STATE_IDLE

#define APP_ISO7816_PWR_STATE_IDLE HAL_ISO7816_PWR_STATE_IDLE

Idle

Definition at line 124 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_OFF

#define APP_ISO7816_PWR_STATE_OFF HAL_ISO7816_PWR_STATE_OFF

Off

Definition at line 116 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_PWRDN_RST

#define APP_ISO7816_PWR_STATE_PWRDN_RST HAL_ISO7816_PWR_STATE_PWRDN_RST

Power Down reset

Definition at line 119 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_PWRDN_VCC

#define APP_ISO7816_PWR_STATE_PWRDN_VCC HAL_ISO7816_PWR_STATE_PWRDN_VCC

Power Down VCC

Definition at line 120 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_PWRUP_RST

#define APP_ISO7816_PWR_STATE_PWRUP_RST HAL_ISO7816_PWR_STATE_PWRUP_RST

Power up reset

Definition at line 118 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_PWRUP_VCC

#define APP_ISO7816_PWR_STATE_PWRUP_VCC HAL_ISO7816_PWR_STATE_PWRUP_VCC

Power up VCC

Definition at line 117 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_RX

#define APP_ISO7816_PWR_STATE_RX HAL_ISO7816_PWR_STATE_RX

Receive

Definition at line 127 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_RX_TS0

#define APP_ISO7816_PWR_STATE_RX_TS0 HAL_ISO7816_PWR_STATE_RX_TS0

RX TS Character

Definition at line 125 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_RX_TS1

#define APP_ISO7816_PWR_STATE_RX_TS1 HAL_ISO7816_PWR_STATE_RX_TS1

RX TS Character

Definition at line 126 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_STOP

#define APP_ISO7816_PWR_STATE_STOP HAL_ISO7816_PWR_STATE_STOP

Clock Stopped

Definition at line 122 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_STOP_POST

#define APP_ISO7816_PWR_STATE_STOP_POST HAL_ISO7816_PWR_STATE_STOP_POST

Exiting Clock Stop

Definition at line 123 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_STOP_PRE

#define APP_ISO7816_PWR_STATE_STOP_PRE HAL_ISO7816_PWR_STATE_STOP_PRE

Preparing Clock Stop

Definition at line 121 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_TX

#define APP_ISO7816_PWR_STATE_TX HAL_ISO7816_PWR_STATE_TX

Transmit

Definition at line 128 of file app_iso7816.h.

## ◆ APP_ISO7816_PWR_STATE_TX_RX

#define APP_ISO7816_PWR_STATE_TX_RX HAL_ISO7816_PWR_STATE_TX_RX

Transmit and Receive

Definition at line 129 of file app_iso7816.h.