Macros
COMP REF SOURCE
Peripheral Driver » LL Driver » COMP » Defines » COMP Exported Constants

## Macros
#define | LL_COMP_REF_SRC_IO0 (0UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)
#define | LL_COMP_REF_SRC_IO1 (1UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)
#define | LL_COMP_REF_SRC_IO2 (2UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)
#define | LL_COMP_REF_SRC_IO3 (3UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)
#define | LL_COMP_REF_SRC_IO4 (4UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)
#define | LL_COMP_REF_SRC_VBAT (6UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)
#define | LL_COMP_REF_SRC_VREF (7UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

## Detailed Description

## Macro Definition Documentation

## ◆ LL_COMP_REF_SRC_IO0

#define LL_COMP_REF_SRC_IO0 (0UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

Set MSIO_0 as references for the comparator

Definition at line 122 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_REF_SRC_IO1

#define LL_COMP_REF_SRC_IO1 (1UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

Set MSIO_1 as references for the comparator

Definition at line 123 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_REF_SRC_IO2

#define LL_COMP_REF_SRC_IO2 (2UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

Set MSIO_2 as references for the comparator

Definition at line 124 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_REF_SRC_IO3

#define LL_COMP_REF_SRC_IO3 (3UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

Set MSIO_3 as references for the comparator

Definition at line 125 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_REF_SRC_IO4

#define LL_COMP_REF_SRC_IO4 (4UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

Set MSIO_4 as references for the comparator

Definition at line 126 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_REF_SRC_VBAT

#define LL_COMP_REF_SRC_VBAT (6UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

Set VBATT as references for the comparator

Definition at line 127 of file gr55xx_ll_comp.h.

## ◆ LL_COMP_REF_SRC_VREF

#define LL_COMP_REF_SRC_VREF (7UL << AON_RF_REG_10_CHANNEL_SEL_N_Pos)

Set VREF as references for the comparator

Definition at line 128 of file gr55xx_ll_comp.h.