Functions
IRQ Handler and Callbacks
Peripheral Driver » HAL Driver » COMP » Functions

IRQ Handler and Callbacks functions. More...

## Functions
void | hal_comp_irq_handler (comp_handle_t *p_comp)
| Handle COMP interrupt request. More...
void | hal_comp_rising_trigger_callback (comp_handle_t *p_comp)
| comparator rising callback. More...
void | hal_comp_falling_trigger_callback (comp_handle_t *p_comp)
| comparator rising callback. More...

## Detailed Description

IRQ Handler and Callbacks functions.

## Function Documentation

## ◆ hal_comp_falling_trigger_callback()

void hal_comp_falling_trigger_callback | ( | comp_handle_t * | p_comp | ) |

comparator rising callback.

Note
  This function should not be modified. When the callback is needed, the hal_comp_falling_trigger_callback can be implemented in the user file.

Parameters

  [in] | p_comp | Pointer to a COMP handle which contains the configuration information for the specified COMP module.

## ◆ hal_comp_irq_handler()

void hal_comp_irq_handler | ( | comp_handle_t * | p_comp | ) |

Handle COMP interrupt request.

Parameters

  [in] | p_comp | Pointer to a COMP handle which contains the configuration information for the specified COMP module.

## ◆ hal_comp_rising_trigger_callback()

void hal_comp_rising_trigger_callback | ( | comp_handle_t * | p_comp | ) |

comparator rising callback.

Note
  This function should not be modified. When the callback is needed, the hal_comp_rising_trigger_callback can be implemented in the user file.

Parameters

  [in] | p_comp | Pointer to a COMP handle which contains the configuration information for the specified COMP module.