Macros
EFUSE Loyout Map
Peripheral Driver » HAL Driver » EFUSE » Defines » EFUSE Exported Macros

## Macros
#define | EFUSE_LAYOUT_UID_FAB (0x00)
#define | EFUSE_LAYOUT_UID_YEAR (0x03)
#define | EFUSE_LAYOUT_UID_MON (0x04)
#define | EFUSE_LAYOUT_UID_LOT_ID (0x05)
#define | EFUSE_LAYOUT_UID_WAFER_ID (0x0D)
#define | EFUSE_LAYOUT_UID_WAFER_X (0x0E)
#define | EFUSE_LAYOUT_UID_WAFER_Y (0x0F)
#define | EFUSE_LAYOUT_FLASH_SE_ADDR1 (0x10)
#define | EFUSE_LAYOUT_FLASH_SE_ADDR2 (0x14)
#define | EFUSE_LAYOUT_USER_START (0x18)
#define | EFUSE_LAYOUT_USER_END (0x1F)

## Detailed Description

## Macro Definition Documentation

## ◆ EFUSE_LAYOUT_FLASH_SE_ADDR1

#define EFUSE_LAYOUT_FLASH_SE_ADDR1 (0x10)

start address for Flash security registers 1

Definition at line 176 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_FLASH_SE_ADDR2

#define EFUSE_LAYOUT_FLASH_SE_ADDR2 (0x14)

start address for Flash security registers 2

Definition at line 177 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_UID_FAB

#define EFUSE_LAYOUT_UID_FAB (0x00)

Store UID-FAB information

Definition at line 168 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_UID_LOT_ID

#define EFUSE_LAYOUT_UID_LOT_ID (0x05)

Store LOT ID information

Definition at line 171 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_UID_MON

#define EFUSE_LAYOUT_UID_MON (0x04)

Store month information

Definition at line 170 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_UID_WAFER_ID

#define EFUSE_LAYOUT_UID_WAFER_ID (0x0D)

Store Wafer ID information

Definition at line 172 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_UID_WAFER_X

#define EFUSE_LAYOUT_UID_WAFER_X (0x0E)

Store Wafer X information

Definition at line 173 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_UID_WAFER_Y

#define EFUSE_LAYOUT_UID_WAFER_Y (0x0F)

Store Wafer Y information

Definition at line 174 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_UID_YEAR

#define EFUSE_LAYOUT_UID_YEAR (0x03)

Store Year information

Definition at line 169 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_USER_END

#define EFUSE_LAYOUT_USER_END (0x1F)

end address for user eFuse space

Definition at line 180 of file hal_efuse.h.

## ◆ EFUSE_LAYOUT_USER_START

#define EFUSE_LAYOUT_USER_START (0x18)

start address for user eFuse space

Definition at line 179 of file hal_efuse.h.